Arduino - Double

Arduino

Guide

Tutorials

Reference

Hardware

Software

Forum

Playground

Exhibition

Hacking

FAQ

Buy

Language | Libraries | Comparison

## double

#### Desciption

Double precision floating point number. Occupies 8 bytes. The maximum value a double can represent is 1.7976931348623157 x 10^308. Yes that's 10 to the 308th power. Just in case you get your Arduino project a spot as a space shuttle experiment.

#### See:

- Float

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

Edit Page | Page History | Printable View | Recent Site Changes