Arduino - EEPROM

Arduino

Guide

Tutorials

Reference

Hardware

Software

Forum

Playground

Exhibition

Hacking

FAQ

Buy

Language | Libraries | Comparison

## EEPROM Library

The microcontroller on the Arduino board has 512 bytes of EEPROM: memory whose values are kept when the board is turned off (like a tiny hard drive). This library enables you to read and write those bytes.

#### Functions

- byte EEPROM.read(address)
- EEPROM.write(address, value)

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

Edit Page | Page History | Printable View | Recent Site Changes