Arduino - LiquidCrystal

Arduino

Buy | Download | Getting Started | Learning | Reference | Hardware | FAQ

Blog » | Forum » | Playground »

Reference Language (extended) | Libraries | Comparison | Board

## LiquidCrystal Library

This library allows an Arduino board to control LiquidCrystal displays (LCDs) based on the XXX chipset, which is found on most text-based LCDs. The library works with in either 4- or 8-bit mode (i.e. using 4 or 8 data lines in addition to the rs, rw, and enable control lines).

#### Function

- LiquidCrystal()
- clear()
- home()
- setCursor()
- write()
- print()

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

Edit Page | Page History | Printable View | All Recent Site Changes