Committed
Binutils 2.19
--------------------------------------------------------------------------------
--- gas/config/tc-avr.c.old	2007-10-09 09:04:20.265625000 -0600
+++ gas/config/tc-avr.c	2007-10-09 09:05:46.312500000 -0600
@@ -115,7 +115,9 @@ static struct mcu_type_s mcu_types[] =
   {"atmega8hva", AVR_ISA_PWMx,    bfd_mach_avr4},
   {"at90pwm1",   AVR_ISA_PWMx,    bfd_mach_avr4},
   {"at90pwm2",   AVR_ISA_PWMx,    bfd_mach_avr4},
+  {"at90pwm2b",  AVR_ISA_PWMx,    bfd_mach_avr4},
   {"at90pwm3",   AVR_ISA_PWMx,    bfd_mach_avr4},
+  {"at90pwm3b",  AVR_ISA_PWMx,    bfd_mach_avr4},
   {"atmega16",   AVR_ISA_M323,    bfd_mach_avr5},
   {"atmega161",  AVR_ISA_M161,    bfd_mach_avr5},
   {"atmega162",  AVR_ISA_M323,    bfd_mach_avr5},
--- gas/doc/c-avr.texi.old	2007-10-09 09:09:03.468750000 -0600
+++ gas/doc/c-avr.texi	2007-10-09 09:09:27.859375000 -0600
@@ -49,7 +49,8 @@ at76c711).
 
 Instruction set avr4 is for the enhanced AVR core with up to 8K program
 memory space (MCU types: atmega48, atmega8, atmega83, atmega85, atmega88,
-atmega8515, atmega8535, atmega8hva, at90pwm1, at90pwm2, at90pwm3).
+atmega8515, atmega8535, atmega8hva, at90pwm1, at90pwm2, at90pwm2b,
+at90pwm3, at90pwm3b).
 
 Instruction set avr5 is for the enhanced AVR core with up to 128K program
 memory space (MCU types: atmega16, atmega161, atmega162, atmega163,
