Committed
Binutils 2.19
--------------------------------------------------------------------------------
Index: gas/config/tc-avr.c
===================================================================
RCS file: /cvs/src/src/gas/config/tc-avr.c,v
retrieving revision 1.44
diff -u -r1.44 tc-avr.c
--- gas/config/tc-avr.c	31 Oct 2007 18:11:28 -0000	1.44
+++ gas/config/tc-avr.c	1 Nov 2007 07:24:12 -0000
@@ -103,8 +103,10 @@
   {"at43usb355", AVR_ISA_M603,    bfd_mach_avr3},
   {"at76c711",   AVR_ISA_M603,    bfd_mach_avr3},
   {"atmega48",   AVR_ISA_PWMx,    bfd_mach_avr4},
+  {"atmega48p",  AVR_ISA_PWMx,    bfd_mach_avr4},
   {"atmega8",    AVR_ISA_M8,      bfd_mach_avr4},
   {"atmega88",   AVR_ISA_PWMx,    bfd_mach_avr4},
+  {"atmega88p",  AVR_ISA_PWMx,    bfd_mach_avr4},
   {"atmega8515", AVR_ISA_M8,      bfd_mach_avr4},
   {"atmega8535", AVR_ISA_M8,      bfd_mach_avr4},
   {"atmega8hva", AVR_ISA_PWMx,    bfd_mach_avr4},
@@ -121,6 +123,7 @@
   {"atmega165",  AVR_ISA_M323,    bfd_mach_avr5},
   {"atmega165p", AVR_ISA_M323,    bfd_mach_avr5},
   {"atmega168",  AVR_ISA_M323,    bfd_mach_avr5},
+  {"atmega168p", AVR_ISA_M323,    bfd_mach_avr5},
   {"atmega169",  AVR_ISA_M323,    bfd_mach_avr5},
   {"atmega169p", AVR_ISA_M323,    bfd_mach_avr5},
   {"atmega32",   AVR_ISA_M323,    bfd_mach_avr5},
@@ -128,6 +131,7 @@
   {"atmega324p", AVR_ISA_M323,    bfd_mach_avr5},
   {"atmega325",  AVR_ISA_M323,    bfd_mach_avr5},
   {"atmega325p", AVR_ISA_M323,    bfd_mach_avr5},
+  {"atmega328p", AVR_ISA_M323,    bfd_mach_avr5},
   {"atmega329",  AVR_ISA_M323,    bfd_mach_avr5},
   {"atmega329p", AVR_ISA_M323,    bfd_mach_avr5},
   {"atmega3250", AVR_ISA_M323,    bfd_mach_avr5},
--- gas/doc/c-avr.texi.old	2007-11-02 10:30:57.213499800 -0600
+++ gas/doc/c-avr.texi	2007-11-02 10:34:24.557249800 -0600
@@ -44,24 +44,23 @@ attiny261, attiny461, attiny861, attiny2
 attiny45, attiny85, attiny43u, attiny48).
 
 Instruction set avr3 is for the classic AVR core with up to 128K program
-memory space (MCU types: atmega103, at43usb320, at43usb355,
-at76c711).
+memory space (MCU types: atmega103, at43usb320, at43usb355, at76c711).
 
 Instruction set avr4 is for the enhanced AVR core with up to 8K program
-memory space (MCU types: atmega48, atmega8, atmega88,
+memory space (MCU types: atmega48, atmega48p atmega8, atmega88, atmega88p,
 atmega8515, atmega8535, atmega8hva, at90pwm1, at90pwm2, at90pwm2b,
 at90pwm3, at90pwm3b).
 
 Instruction set avr5 is for the enhanced AVR core with up to 128K program
 memory space (MCU types: atmega16, atmega161, atmega162, atmega163,
-atmega164p, atmega165, atmega165p, atmega168, atmega169, atmega169p, 
-atmega32, atmega323, atmega324p, atmega325, atmega325p, atmega329, 
-atmega329p, atmega3250, atmega3250p, atmega3290, atmega3290p, atmega406, 
-atmega64, atmega640, atmega644, atmega644p, atmega128, atmega1280, 
-atmega1281, atmega645, atmega649, atmega6450, atmega6490, atmega16hva, 
-at90can32, at90can64, at90can128, at90pwm216, at90pwm316, 
-at90usb82, at90usb162, at90usb646, 
-at90usb647, at90usb1286, at90usb1287, at94k).
+atmega164p, atmega165, atmega165p, atmega168, atmega168p, atmega169, 
+atmega169p, atmega32, atmega323, atmega324p, atmega325, atmega325p, 
+atmega328p, atmega329, atmega329p, atmega3250, atmega3250p, atmega3290, 
+atmega3290p, atmega406, atmega64, atmega640, atmega644, atmega644p, 
+atmega128, atmega1280, atmega1281, atmega645, atmega649, atmega6450, 
+atmega6490, atmega16hva, at90can32, at90can64, at90can128, at90pwm216, 
+at90pwm316, at90usb82, at90usb162, at90usb646, at90usb647, at90usb1286, 
+at90usb1287, at94k).
 
 Instruction set avr6 is for the enhanced AVR core with 256K program
 memory space (MCU types: atmega2560, atmega2561).
