Arduino - SoftwareSerialBegin

Arduino

Buy | Download | Getting Started | Learning | Reference | Hardware | FAQ

Blog » | Forum » | Playground »

Reference Language (extended) | Libraries | Comparison | Board

## SoftwareSerial: begin(speed)

#### Description

Sets the speed (baud rate) for the serial communication. Using speeds higher than 9600 baud will result in faulty communication.

#### Parameters

speed: the baud rate (long)

#### Returns

none

#### Example

    // include the SoftwareSerial library so you can use its functions:
    #include <SoftwareSerial.h>

    #define rxPin 2
    #define txPin 3

    // set up a new serial port
    SoftwareSerial mySerial =  SoftwareSerial(rxPin, txPin);

    void setup()  {
      // define pin modes for tx, rx:
      pinMode(rxPin, INPUT);
      pinMode(txPin, OUTPUT);
      // set the data rate for the SoftwareSerial port
      mySerial.begin(9600);
    }

    void loop() {
      // ...
    }

#### See also

- SoftwareSerial()
- read()
- print()
- println()

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

Edit Page | Page History | Printable View | All Recent Site Changes