Arduino - Double

Arduino

Buy | Download | Getting Started | Learning | Reference | Hardware | FAQ

Blog » | Forum » | Playground »

Reference Language (extended) | Libraries | Comparison | Board

## double

#### Desciption

Double precision floating point number. Occupies 4 bytes. The maximum value a double can represent is 1.7976931348623157 x 10^308. (2^64 - 1)

#### See:

- Float

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

Edit Page | Page History | Printable View | All Recent Site Changes