Arduino - LiquidCrystalPrint

Arduino

Buy | Download | Getting Started | Learning | Reference | Hardware | FAQ

Blog » | Forum » | Playground »

Reference Language (extended) | Libraries | Comparison | Board

LiquidCrystal

## print()

#### Description

Prints text to the LCD.

#### Syntax

lcd.print(data)
lcd.print(data, BASE)

#### Parameters

lcd: a variable of type LiquidCrystal

data: the data to print (char, byte, int, long, or string)

BASE (optional): the base in which to print numbers: BIN for binary (base 2), DEC for decimal (base 10), OCT for octal (base 8), HEX for hexadecimal (base 16).

#### Example

    #include <LiquidCrystal.h>

    LiquidCrystal lcd(12, 11, 10, 5, 4, 3, 2);

    void setup()
    {
      lcd.print("hello, world!");
    }

    void loop() {}

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

Edit Page | Page History | Printable View | All Recent Site Changes