Arduino - Continue

Arduino

Buy | Download | Getting Started | Learning | Reference | Hardware | FAQ

Blog » | Forum » | Playground »

Reference Language (extended) | Libraries | Comparison | Board

## continue

continue is used to bypass portions of code in a do, for, or while loop. It forces the conditional expression to be evaluated, without terminating the loop.

#### Example

    for (x = 0; x < 255; x ++)
    {
        if (x > 40 && x < 120){      // create jump in values
            continue;
        }

        digitalWrite(PWMpin, x);
        delay(50);
    }

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

Edit Page | Page History | Printable View | All Recent Site Changes