This is libc.info, produced by makeinfo version 4.0b from libc.texinfo.

INFO-DIR-SECTION GNU libraries
START-INFO-DIR-ENTRY
* Libc: (libc).                 C library.
END-INFO-DIR-ENTRY

   This file documents the GNU C library.

   This is Edition 0.10, last updated 2001-07-06, of `The GNU C Library
Reference Manual', for Version 2.2.x.

   Copyright (C) 1993, 1994, 1995, 1996, 1997, 1998, 1999, 2001 Free
Software Foundation, Inc.

   Permission is granted to copy, distribute and/or modify this document
under the terms of the GNU Free Documentation License, Version 1.1 or
any later version published by the Free Software Foundation; with the
Invariant Sections being "GNU Lesser General Public License", the
Front-Cover texts being (a) (see below), and with the Back-Cover Texts
being (b) (see below).  A copy of the license is included in the section
entitled "GNU Free Documentation License".

   (a) The FSF's Front-Cover Text is:

   A GNU Manual

   (b) The FSF's Back-Cover Text is:

   You have freedom to copy and modify this GNU Manual, like GNU
software.  Copies published by the Free Software Foundation raise
funds for GNU development.


File: libc.info,  Node: Socket Option Functions,  Next: Socket-Level Options,  Up: Socket Options

Socket Option Functions
-----------------------

   Here are the functions for examining and modifying socket options.
They are declared in `sys/socket.h'.

 - Function: int getsockopt (int SOCKET, int LEVEL, int OPTNAME, void
          *OPTVAL, socklen_t *OPTLEN-PTR)
     The `getsockopt' function gets information about the value of
     option OPTNAME at level LEVEL for socket SOCKET.

     The option value is stored in a buffer that OPTVAL points to.
     Before the call, you should supply in `*OPTLEN-PTR' the size of
     this buffer; on return, it contains the number of bytes of
     information actually stored in the buffer.

     Most options interpret the OPTVAL buffer as a single `int' value.

     The actual return value of `getsockopt' is `0' on success and `-1'
     on failure.  The following `errno' error conditions are defined:

    `EBADF'
          The SOCKET argument is not a valid file descriptor.

    `ENOTSOCK'
          The descriptor SOCKET is not a socket.

    `ENOPROTOOPT'
          The OPTNAME doesn't make sense for the given LEVEL.

 - Function: int setsockopt (int SOCKET, int LEVEL, int OPTNAME, void
          *OPTVAL, socklen_t OPTLEN)
     This function is used to set the socket option OPTNAME at level
     LEVEL for socket SOCKET.  The value of the option is passed in the
     buffer OPTVAL of size OPTLEN.

     The return value and error codes for `setsockopt' are the same as
     for `getsockopt'.



File: libc.info,  Node: Socket-Level Options,  Prev: Socket Option Functions,  Up: Socket Options

Socket-Level Options
--------------------

 - Constant: int SOL_SOCKET
     Use this constant as the LEVEL argument to `getsockopt' or
     `setsockopt' to manipulate the socket-level options described in
     this section.

Here is a table of socket-level option names; all are defined in the
header file `sys/socket.h'.

`SO_DEBUG'
     This option toggles recording of debugging information in the
     underlying protocol modules.  The value has type `int'; a nonzero
     value means "yes".

`SO_REUSEADDR'
     This option controls whether `bind' (*note Setting Address::)
     should permit reuse of local addresses for this socket.  If you
     enable this option, you can actually have two sockets with the
     same Internet port number; but the system won't allow you to use
     the two identically-named sockets in a way that would confuse the
     Internet.  The reason for this option is that some higher-level
     Internet protocols, including FTP, require you to keep reusing the
     same port number.

     The value has type `int'; a nonzero value means "yes".

`SO_KEEPALIVE'
     This option controls whether the underlying protocol should
     periodically transmit messages on a connected socket.  If the peer
     fails to respond to these messages, the connection is considered
     broken.  The value has type `int'; a nonzero value means "yes".

`SO_DONTROUTE'
     This option controls whether outgoing messages bypass the normal
     message routing facilities.  If set, messages are sent directly to
     the network interface instead.  The value has type `int'; a nonzero
     value means "yes".

`SO_LINGER'
     This option specifies what should happen when the socket of a type
     that promises reliable delivery still has untransmitted messages
     when it is closed; see *Note Closing a Socket::.  The value has
     type `struct linger'.

      - Data Type: struct linger
          This structure type has the following members:

         `int l_onoff'
               This field is interpreted as a boolean.  If nonzero,
               `close' blocks until the data are transmitted or the
               timeout period has expired.

         `int l_linger'
               This specifies the timeout period, in seconds.

`SO_BROADCAST'
     This option controls whether datagrams may be broadcast from the
     socket.  The value has type `int'; a nonzero value means "yes".

`SO_OOBINLINE'
     If this option is set, out-of-band data received on the socket is
     placed in the normal input queue.  This permits it to be read using
     `read' or `recv' without specifying the `MSG_OOB' flag.  *Note
     Out-of-Band Data::.  The value has type `int'; a nonzero value
     means "yes".

`SO_SNDBUF'
     This option gets or sets the size of the output buffer.  The value
     is a `size_t', which is the size in bytes.

`SO_RCVBUF'
     This option gets or sets the size of the input buffer.  The value
     is a `size_t', which is the size in bytes.

`SO_STYLE'
`SO_TYPE'
     This option can be used with `getsockopt' only.  It is used to get
     the socket's communication style.  `SO_TYPE' is the historical
     name, and `SO_STYLE' is the preferred name in GNU.  The value has
     type `int' and its value designates a communication style; see
     *Note Communication Styles::.

`SO_ERROR'
     This option can be used with `getsockopt' only.  It is used to
     reset the error status of the socket.  The value is an `int',
     which represents the previous error status.


File: libc.info,  Node: Networks Database,  Prev: Socket Options,  Up: Sockets

Networks Database
=================

   Many systems come with a database that records a list of networks
known to the system developer.  This is usually kept either in the file
`/etc/networks' or in an equivalent from a name server.  This data base
is useful for routing programs such as `route', but it is not useful
for programs that simply communicate over the network.  We provide
functions to access this database, which are declared in `netdb.h'.

 - Data Type: struct netent
     This data type is used to represent information about entries in
     the networks database.  It has the following members:

    `char *n_name'
          This is the "official" name of the network.

    `char **n_aliases'
          These are alternative names for the network, represented as a
          vector of strings.  A null pointer terminates the array.

    `int n_addrtype'
          This is the type of the network number; this is always equal
          to `AF_INET' for Internet networks.

    `unsigned long int n_net'
          This is the network number.  Network numbers are returned in
          host byte order; see *Note Byte Order::.

   Use the `getnetbyname' or `getnetbyaddr' functions to search the
networks database for information about a specific network.  The
information is returned in a statically-allocated structure; you must
copy the information if you need to save it.

 - Function: struct netent * getnetbyname (const char *NAME)
     The `getnetbyname' function returns information about the network
     named NAME.  It returns a null pointer if there is no such network.

 - Function: struct netent * getnetbyaddr (unsigned long int NET, int
          TYPE)
     The `getnetbyaddr' function returns information about the network
     of type TYPE with number NET.  You should specify a value of
     `AF_INET' for the TYPE argument for Internet networks.

     `getnetbyaddr' returns a null pointer if there is no such network.

   You can also scan the networks database using `setnetent',
`getnetent' and `endnetent'.  Be careful when using these functions
because they are not reentrant.

 - Function: void setnetent (int STAYOPEN)
     This function opens and rewinds the networks database.

     If the STAYOPEN argument is nonzero, this sets a flag so that
     subsequent calls to `getnetbyname' or `getnetbyaddr' will not
     close the database (as they usually would).  This makes for more
     efficiency if you call those functions several times, by avoiding
     reopening the database for each call.

 - Function: struct netent * getnetent (void)
     This function returns the next entry in the networks database.  It
     returns a null pointer if there are no more entries.

 - Function: void endnetent (void)
     This function closes the networks database.


File: libc.info,  Node: Low-Level Terminal Interface,  Next: Syslog,  Prev: Sockets,  Up: Top

Low-Level Terminal Interface
****************************

   This chapter describes functions that are specific to terminal
devices.  You can use these functions to do things like turn off input
echoing; set serial line characteristics such as line speed and flow
control; and change which characters are used for end-of-file,
command-line editing, sending signals, and similar control functions.

   Most of the functions in this chapter operate on file descriptors.
*Note Low-Level I/O::, for more information about what a file
descriptor is and how to open a file descriptor for a terminal device.

* Menu:

* Is It a Terminal::            How to determine if a file is a terminal
			         device, and what its name is.
* I/O Queues::                  About flow control and typeahead.
* Canonical or Not::            Two basic styles of input processing.
* Terminal Modes::              How to examine and modify flags controlling
			         details of terminal I/O: echoing,
                                 signals, editing.  Posix.
* BSD Terminal Modes::          BSD compatible terminal mode setting
* Line Control::                Sending break sequences, clearing
                                 terminal buffers ...
* Noncanon Example::            How to read single characters without echo.
* Pseudo-Terminals::            How to open a pseudo-terminal.


File: libc.info,  Node: Is It a Terminal,  Next: I/O Queues,  Up: Low-Level Terminal Interface

Identifying Terminals
=====================

   The functions described in this chapter only work on files that
correspond to terminal devices.  You can find out whether a file
descriptor is associated with a terminal by using the `isatty' function.

   Prototypes for the functions in this section are declared in the
header file `unistd.h'.

 - Function: int isatty (int FILEDES)
     This function returns `1' if FILEDES is a file descriptor
     associated with an open terminal device, and 0 otherwise.

   If a file descriptor is associated with a terminal, you can get its
associated file name using the `ttyname' function.  See also the
`ctermid' function, described in *Note Identifying the Terminal::.

 - Function: char * ttyname (int FILEDES)
     If the file descriptor FILEDES is associated with a terminal
     device, the `ttyname' function returns a pointer to a
     statically-allocated, null-terminated string containing the file
     name of the terminal file.  The value is a null pointer if the
     file descriptor isn't associated with a terminal, or the file name
     cannot be determined.

 - Function: int ttyname_r (int FILEDES, char *BUF, size_t LEN)
     The `ttyname_r' function is similar to the `ttyname' function
     except that it places its result into the user-specified buffer
     starting at BUF with length LEN.

     The normal return value from `ttyname_r' is 0.  Otherwise an error
     number is returned to indicate the error.  The following `errno'
     error conditions are defined for this function:

    `EBADF'
          The FILEDES argument is not a valid file descriptor.

    `ENOTTY'
          The FILEDES is not associated with a terminal.

    `ERANGE'
          The buffer length LEN is too small to store the string to be
          returned.


File: libc.info,  Node: I/O Queues,  Next: Canonical or Not,  Prev: Is It a Terminal,  Up: Low-Level Terminal Interface

I/O Queues
==========

   Many of the remaining functions in this section refer to the input
and output queues of a terminal device.  These queues implement a form
of buffering _within the kernel_ independent of the buffering
implemented by I/O streams (*note I/O on Streams::).

   The "terminal input queue" is also sometimes referred to as its
"typeahead buffer".  It holds the characters that have been received
from the terminal but not yet read by any process.

   The size of the input queue is described by the `MAX_INPUT' and
`_POSIX_MAX_INPUT' parameters; see *Note Limits for Files::.  You are
guaranteed a queue size of at least `MAX_INPUT', but the queue might be
larger, and might even dynamically change size.  If input flow control
is enabled by setting the `IXOFF' input mode bit (*note Input Modes::),
the terminal driver transmits STOP and START characters to the terminal
when necessary to prevent the queue from overflowing.  Otherwise, input
may be lost if it comes in too fast from the terminal.  In canonical
mode, all input stays in the queue until a newline character is
received, so the terminal input queue can fill up when you type a very
long line.  *Note Canonical or Not::.

   The "terminal output queue" is like the input queue, but for output;
it contains characters that have been written by processes, but not yet
transmitted to the terminal.  If output flow control is enabled by
setting the `IXON' input mode bit (*note Input Modes::), the terminal
driver obeys START and STOP characters sent by the terminal to stop and
restart transmission of output.

   "Clearing" the terminal input queue means discarding any characters
that have been received but not yet read.  Similarly, clearing the
terminal output queue means discarding any characters that have been
written but not yet transmitted.


File: libc.info,  Node: Canonical or Not,  Next: Terminal Modes,  Prev: I/O Queues,  Up: Low-Level Terminal Interface

Two Styles of Input: Canonical or Not
=====================================

   POSIX systems support two basic modes of input: canonical and
noncanonical.

   In "canonical input processing" mode, terminal input is processed in
lines terminated by newline (`'\n''), EOF, or EOL characters.  No input
can be read until an entire line has been typed by the user, and the
`read' function (*note I/O Primitives::) returns at most a single line
of input, no matter how many bytes are requested.

   In canonical input mode, the operating system provides input editing
facilities: some characters are interpreted specially to perform editing
operations within the current line of text, such as ERASE and KILL.
*Note Editing Characters::.

   The constants `_POSIX_MAX_CANON' and `MAX_CANON' parameterize the
maximum number of bytes which may appear in a single line of canonical
input.  *Note Limits for Files::.  You are guaranteed a maximum line
length of at least `MAX_CANON' bytes, but the maximum might be larger,
and might even dynamically change size.

   In "noncanonical input processing" mode, characters are not grouped
into lines, and ERASE and KILL processing is not performed.  The
granularity with which bytes are read in noncanonical input mode is
controlled by the MIN and TIME settings.  *Note Noncanonical Input::.

   Most programs use canonical input mode, because this gives the user a
way to edit input line by line.  The usual reason to use noncanonical
mode is when the program accepts single-character commands or provides
its own editing facilities.

   The choice of canonical or noncanonical input is controlled by the
`ICANON' flag in the `c_lflag' member of `struct termios'.  *Note Local
Modes::.


File: libc.info,  Node: Terminal Modes,  Next: BSD Terminal Modes,  Prev: Canonical or Not,  Up: Low-Level Terminal Interface

Terminal Modes
==============

   This section describes the various terminal attributes that control
how input and output are done.  The functions, data structures, and
symbolic constants are all declared in the header file `termios.h'.

   Don't confuse terminal attributes with file attributes.  A device
special file which is associated with a terminal has file attributes as
described in *Note File Attributes::.  These are unrelated to the
attributes of the terminal device itself, which are discussed in this
section.

* Menu:

* Mode Data Types::             The data type `struct termios' and
                                 related types.
* Mode Functions::              Functions to read and set the terminal
                                 attributes.
* Setting Modes::               The right way to set terminal attributes
                                 reliably.
* Input Modes::                 Flags controlling low-level input handling.
* Output Modes::                Flags controlling low-level output handling.
* Control Modes::               Flags controlling serial port behavior.
* Local Modes::                 Flags controlling high-level input handling.
* Line Speed::                  How to read and set the terminal line speed.
* Special Characters::          Characters that have special effects,
			         and how to change them.
* Noncanonical Input::          Controlling how long to wait for input.


File: libc.info,  Node: Mode Data Types,  Next: Mode Functions,  Up: Terminal Modes

Terminal Mode Data Types
------------------------

   The entire collection of attributes of a terminal is stored in a
structure of type `struct termios'.  This structure is used with the
functions `tcgetattr' and `tcsetattr' to read and set the attributes.

 - Data Type: struct termios
     Structure that records all the I/O attributes of a terminal.  The
     structure includes at least the following members:

    `tcflag_t c_iflag'
          A bit mask specifying flags for input modes; see *Note Input
          Modes::.

    `tcflag_t c_oflag'
          A bit mask specifying flags for output modes; see *Note
          Output Modes::.

    `tcflag_t c_cflag'
          A bit mask specifying flags for control modes; see *Note
          Control Modes::.

    `tcflag_t c_lflag'
          A bit mask specifying flags for local modes; see *Note Local
          Modes::.

    `cc_t c_cc[NCCS]'
          An array specifying which characters are associated with
          various control functions; see *Note Special Characters::.

     The `struct termios' structure also contains members which encode
     input and output transmission speeds, but the representation is
     not specified.  *Note Line Speed::, for how to examine and store
     the speed values.

   The following sections describe the details of the members of the
`struct termios' structure.

 - Data Type: tcflag_t
     This is an unsigned integer type used to represent the various bit
     masks for terminal flags.

 - Data Type: cc_t
     This is an unsigned integer type used to represent characters
     associated with various terminal control functions.

 - Macro: int NCCS
     The value of this macro is the number of elements in the `c_cc'
     array.


File: libc.info,  Node: Mode Functions,  Next: Setting Modes,  Prev: Mode Data Types,  Up: Terminal Modes

Terminal Mode Functions
-----------------------

 - Function: int tcgetattr (int FILEDES, struct termios *TERMIOS-P)
     This function is used to examine the attributes of the terminal
     device with file descriptor FILEDES.  The attributes are returned
     in the structure that TERMIOS-P points to.

     If successful, `tcgetattr' returns 0.  A return value of -1
     indicates an error.  The following `errno' error conditions are
     defined for this function:

    `EBADF'
          The FILEDES argument is not a valid file descriptor.

    `ENOTTY'
          The FILEDES is not associated with a terminal.

 - Function: int tcsetattr (int FILEDES, int WHEN, const struct termios
          *TERMIOS-P)
     This function sets the attributes of the terminal device with file
     descriptor FILEDES.  The new attributes are taken from the
     structure that TERMIOS-P points to.

     The WHEN argument specifies how to deal with input and output
     already queued.  It can be one of the following values:

    `TCSANOW'
          Make the change immediately.

    `TCSADRAIN'
          Make the change after waiting until all queued output has
          been written.  You should usually use this option when
          changing parameters that affect output.

    `TCSAFLUSH'
          This is like `TCSADRAIN', but also discards any queued input.

    `TCSASOFT'
          This is a flag bit that you can add to any of the above
          alternatives.  Its meaning is to inhibit alteration of the
          state of the terminal hardware.  It is a BSD extension; it is
          only supported on BSD systems and the GNU system.

          Using `TCSASOFT' is exactly the same as setting the `CIGNORE'
          bit in the `c_cflag' member of the structure TERMIOS-P points
          to.  *Note Control Modes::, for a description of `CIGNORE'.

     If this function is called from a background process on its
     controlling terminal, normally all processes in the process group
     are sent a `SIGTTOU' signal, in the same way as if the process
     were trying to write to the terminal.  The exception is if the
     calling process itself is ignoring or blocking `SIGTTOU' signals,
     in which case the operation is performed and no signal is sent.
     *Note Job Control::.

     If successful, `tcsetattr' returns 0.  A return value of -1
     indicates an error.  The following `errno' error conditions are
     defined for this function:

    `EBADF'
          The FILEDES argument is not a valid file descriptor.

    `ENOTTY'
          The FILEDES is not associated with a terminal.

    `EINVAL'
          Either the value of the `when' argument is not valid, or
          there is something wrong with the data in the TERMIOS-P
          argument.

   Although `tcgetattr' and `tcsetattr' specify the terminal device
with a file descriptor, the attributes are those of the terminal device
itself and not of the file descriptor.  This means that the effects of
changing terminal attributes are persistent; if another process opens
the terminal file later on, it will see the changed attributes even
though it doesn't have anything to do with the open file descriptor you
originally specified in changing the attributes.

   Similarly, if a single process has multiple or duplicated file
descriptors for the same terminal device, changing the terminal
attributes affects input and output to all of these file descriptors.
This means, for example, that you can't open one file descriptor or
stream to read from a terminal in the normal line-buffered, echoed
mode; and simultaneously have another file descriptor for the same
terminal that you use to read from it in single-character, non-echoed
mode.  Instead, you have to explicitly switch the terminal back and
forth between the two modes.


File: libc.info,  Node: Setting Modes,  Next: Input Modes,  Prev: Mode Functions,  Up: Terminal Modes

Setting Terminal Modes Properly
-------------------------------

   When you set terminal modes, you should call `tcgetattr' first to
get the current modes of the particular terminal device, modify only
those modes that you are really interested in, and store the result with
`tcsetattr'.

   It's a bad idea to simply initialize a `struct termios' structure to
a chosen set of attributes and pass it directly to `tcsetattr'.  Your
program may be run years from now, on systems that support members not
documented in this manual.  The way to avoid setting these members to
unreasonable values is to avoid changing them.

   What's more, different terminal devices may require different mode
settings in order to function properly.  So you should avoid blindly
copying attributes from one terminal device to another.

   When a member contains a collection of independent flags, as the
`c_iflag', `c_oflag' and `c_cflag' members do, even setting the entire
member is a bad idea, because particular operating systems have their
own flags.  Instead, you should start with the current value of the
member and alter only the flags whose values matter in your program,
leaving any other flags unchanged.

   Here is an example of how to set one flag (`ISTRIP') in the `struct
termios' structure while properly preserving all the other data in the
structure:

     int
     set_istrip (int desc, int value)
     {
       struct termios settings;
       int result;
     
       result = tcgetattr (desc, &settings);
       if (result < 0)
         {
           perror ("error in tcgetattr");
           return 0;
         }
       settings.c_iflag &= ~ISTRIP;
       if (value)
         settings.c_iflag |= ISTRIP;
       result = tcsetattr (desc, TCSANOW, &settings);
       if (result < 0)
         {
           perror ("error in tcgetattr");
           return;
        }
       return 1;
     }


File: libc.info,  Node: Input Modes,  Next: Output Modes,  Prev: Setting Modes,  Up: Terminal Modes

Input Modes
-----------

   This section describes the terminal attribute flags that control
fairly low-level aspects of input processing: handling of parity errors,
break signals, flow control, and <RET> and <LFD> characters.

   All of these flags are bits in the `c_iflag' member of the `struct
termios' structure.  The member is an integer, and you change flags
using the operators `&', `|' and `^'.  Don't try to specify the entire
value for `c_iflag'--instead, change only specific flags and leave the
rest untouched (*note Setting Modes::).

 - Macro: tcflag_t INPCK
     If this bit is set, input parity checking is enabled.  If it is
     not set, no checking at all is done for parity errors on input; the
     characters are simply passed through to the application.

     Parity checking on input processing is independent of whether
     parity detection and generation on the underlying terminal
     hardware is enabled; see *Note Control Modes::.  For example, you
     could clear the `INPCK' input mode flag and set the `PARENB'
     control mode flag to ignore parity errors on input, but still
     generate parity on output.

     If this bit is set, what happens when a parity error is detected
     depends on whether the `IGNPAR' or `PARMRK' bits are set.  If
     neither of these bits are set, a byte with a parity error is
     passed to the application as a `'\0'' character.

 - Macro: tcflag_t IGNPAR
     If this bit is set, any byte with a framing or parity error is
     ignored.  This is only useful if `INPCK' is also set.

 - Macro: tcflag_t PARMRK
     If this bit is set, input bytes with parity or framing errors are
     marked when passed to the program.  This bit is meaningful only
     when `INPCK' is set and `IGNPAR' is not set.

     The way erroneous bytes are marked is with two preceding bytes,
     `377' and `0'.  Thus, the program actually reads three bytes for
     one erroneous byte received from the terminal.

     If a valid byte has the value `0377', and `ISTRIP' (see below) is
     not set, the program might confuse it with the prefix that marks a
     parity error.  So a valid byte `0377' is passed to the program as
     two bytes, `0377' `0377', in this case.

 - Macro: tcflag_t ISTRIP
     If this bit is set, valid input bytes are stripped to seven bits;
     otherwise, all eight bits are available for programs to read.

 - Macro: tcflag_t IGNBRK
     If this bit is set, break conditions are ignored.

     A "break condition" is defined in the context of asynchronous
     serial data transmission as a series of zero-value bits longer
     than a single byte.

 - Macro: tcflag_t BRKINT
     If this bit is set and `IGNBRK' is not set, a break condition
     clears the terminal input and output queues and raises a `SIGINT'
     signal for the foreground process group associated with the
     terminal.

     If neither `BRKINT' nor `IGNBRK' are set, a break condition is
     passed to the application as a single `'\0'' character if `PARMRK'
     is not set, or otherwise as a three-character sequence `'\377'',
     `'\0'', `'\0''.

 - Macro: tcflag_t IGNCR
     If this bit is set, carriage return characters (`'\r'') are
     discarded on input.  Discarding carriage return may be useful on
     terminals that send both carriage return and linefeed when you
     type the <RET> key.

 - Macro: tcflag_t ICRNL
     If this bit is set and `IGNCR' is not set, carriage return
     characters (`'\r'') received as input are passed to the
     application as newline characters (`'\n'').

 - Macro: tcflag_t INLCR
     If this bit is set, newline characters (`'\n'') received as input
     are passed to the application as carriage return characters
     (`'\r'').

 - Macro: tcflag_t IXOFF
     If this bit is set, start/stop control on input is enabled.  In
     other words, the computer sends STOP and START characters as
     necessary to prevent input from coming in faster than programs are
     reading it.  The idea is that the actual terminal hardware that is
     generating the input data responds to a STOP character by
     suspending transmission, and to a START character by resuming
     transmission.  *Note Start/Stop Characters::.

 - Macro: tcflag_t IXON
     If this bit is set, start/stop control on output is enabled.  In
     other words, if the computer receives a STOP character, it
     suspends output until a START character is received.  In this
     case, the STOP and START characters are never passed to the
     application program.  If this bit is not set, then START and STOP
     can be read as ordinary characters.  *Note Start/Stop Characters::.

 - Macro: tcflag_t IXANY
     If this bit is set, any input character restarts output when
     output has been suspended with the STOP character.  Otherwise,
     only the START character restarts output.

     This is a BSD extension; it exists only on BSD systems and the GNU
     system.

 - Macro: tcflag_t IMAXBEL
     If this bit is set, then filling up the terminal input buffer
     sends a BEL character (code `007') to the terminal to ring the
     bell.

     This is a BSD extension.


File: libc.info,  Node: Output Modes,  Next: Control Modes,  Prev: Input Modes,  Up: Terminal Modes

Output Modes
------------

   This section describes the terminal flags and fields that control how
output characters are translated and padded for display.  All of these
are contained in the `c_oflag' member of the `struct termios' structure.

   The `c_oflag' member itself is an integer, and you change the flags
and fields using the operators `&', `|', and `^'.  Don't try to specify
the entire value for `c_oflag'--instead, change only specific flags and
leave the rest untouched (*note Setting Modes::).

 - Macro: tcflag_t OPOST
     If this bit is set, output data is processed in some unspecified
     way so that it is displayed appropriately on the terminal device.
     This typically includes mapping newline characters (`'\n'') onto
     carriage return and linefeed pairs.

     If this bit isn't set, the characters are transmitted as-is.

   The following three bits are BSD features, and they exist only BSD
systems and the GNU system.  They are effective only if `OPOST' is set.

 - Macro: tcflag_t ONLCR
     If this bit is set, convert the newline character on output into a
     pair of characters, carriage return followed by linefeed.

 - Macro: tcflag_t OXTABS
     If this bit is set, convert tab characters on output into the
     appropriate number of spaces to emulate a tab stop every eight
     columns.

 - Macro: tcflag_t ONOEOT
     If this bit is set, discard `C-d' characters (code `004') on
     output.  These characters cause many dial-up terminals to
     disconnect.


File: libc.info,  Node: Control Modes,  Next: Local Modes,  Prev: Output Modes,  Up: Terminal Modes

Control Modes
-------------

   This section describes the terminal flags and fields that control
parameters usually associated with asynchronous serial data
transmission.  These flags may not make sense for other kinds of
terminal ports (such as a network connection pseudo-terminal).  All of
these are contained in the `c_cflag' member of the `struct termios'
structure.

   The `c_cflag' member itself is an integer, and you change the flags
and fields using the operators `&', `|', and `^'.  Don't try to specify
the entire value for `c_cflag'--instead, change only specific flags and
leave the rest untouched (*note Setting Modes::).

 - Macro: tcflag_t CLOCAL
     If this bit is set, it indicates that the terminal is connected
     "locally" and that the modem status lines (such as carrier detect)
     should be ignored.

     On many systems if this bit is not set and you call `open' without
     the `O_NONBLOCK' flag set, `open' blocks until a modem connection
     is established.

     If this bit is not set and a modem disconnect is detected, a
     `SIGHUP' signal is sent to the controlling process group for the
     terminal (if it has one).  Normally, this causes the process to
     exit; see *Note Signal Handling::.  Reading from the terminal
     after a disconnect causes an end-of-file condition, and writing
     causes an `EIO' error to be returned.  The terminal device must be
     closed and reopened to clear the condition.

 - Macro: tcflag_t HUPCL
     If this bit is set, a modem disconnect is generated when all
     processes that have the terminal device open have either closed
     the file or exited.

 - Macro: tcflag_t CREAD
     If this bit is set, input can be read from the terminal.
     Otherwise, input is discarded when it arrives.

 - Macro: tcflag_t CSTOPB
     If this bit is set, two stop bits are used.  Otherwise, only one
     stop bit is used.

 - Macro: tcflag_t PARENB
     If this bit is set, generation and detection of a parity bit are
     enabled.  *Note Input Modes::, for information on how input parity
     errors are handled.

     If this bit is not set, no parity bit is added to output
     characters, and input characters are not checked for correct
     parity.

 - Macro: tcflag_t PARODD
     This bit is only useful if `PARENB' is set.  If `PARODD' is set,
     odd parity is used, otherwise even parity is used.

   The control mode flags also includes a field for the number of bits
per character.  You can use the `CSIZE' macro as a mask to extract the
value, like this: `settings.c_cflag & CSIZE'.

 - Macro: tcflag_t CSIZE
     This is a mask for the number of bits per character.

 - Macro: tcflag_t CS5
     This specifies five bits per byte.

 - Macro: tcflag_t CS6
     This specifies six bits per byte.

 - Macro: tcflag_t CS7
     This specifies seven bits per byte.

 - Macro: tcflag_t CS8
     This specifies eight bits per byte.

   The following four bits are BSD extensions; this exist only on BSD
systems and the GNU system.

 - Macro: tcflag_t CCTS_OFLOW
     If this bit is set, enable flow control of output based on the CTS
     wire (RS232 protocol).

 - Macro: tcflag_t CRTS_IFLOW
     If this bit is set, enable flow control of input based on the RTS
     wire (RS232 protocol).

 - Macro: tcflag_t MDMBUF
     If this bit is set, enable carrier-based flow control of output.

 - Macro: tcflag_t CIGNORE
     If this bit is set, it says to ignore the control modes and line
     speed values entirely.  This is only meaningful in a call to
     `tcsetattr'.

     The `c_cflag' member and the line speed values returned by
     `cfgetispeed' and `cfgetospeed' will be unaffected by the call.
     `CIGNORE' is useful if you want to set all the software modes in
     the other members, but leave the hardware details in `c_cflag'
     unchanged.  (This is how the `TCSASOFT' flag to `tcsettattr'
     works.)

     This bit is never set in the structure filled in by `tcgetattr'.


File: libc.info,  Node: Local Modes,  Next: Line Speed,  Prev: Control Modes,  Up: Terminal Modes

Local Modes
-----------

   This section describes the flags for the `c_lflag' member of the
`struct termios' structure.  These flags generally control higher-level
aspects of input processing than the input modes flags described in
*Note Input Modes::, such as echoing, signals, and the choice of
canonical or noncanonical input.

   The `c_lflag' member itself is an integer, and you change the flags
and fields using the operators `&', `|', and `^'.  Don't try to specify
the entire value for `c_lflag'--instead, change only specific flags and
leave the rest untouched (*note Setting Modes::).

 - Macro: tcflag_t ICANON
     This bit, if set, enables canonical input processing mode.
     Otherwise, input is processed in noncanonical mode.  *Note
     Canonical or Not::.

 - Macro: tcflag_t ECHO
     If this bit is set, echoing of input characters back to the
     terminal is enabled.

 - Macro: tcflag_t ECHOE
     If this bit is set, echoing indicates erasure of input with the
     ERASE character by erasing the last character in the current line
     from the screen.  Otherwise, the character erased is re-echoed to
     show what has happened (suitable for a printing terminal).

     This bit only controls the display behavior; the `ICANON' bit by
     itself controls actual recognition of the ERASE character and
     erasure of input, without which `ECHOE' is simply irrelevant.

 - Macro: tcflag_t ECHOPRT
     This bit is like `ECHOE', enables display of the ERASE character in
     a way that is geared to a hardcopy terminal.  When you type the
     ERASE character, a `\' character is printed followed by the first
     character erased.  Typing the ERASE character again just prints
     the next character erased.  Then, the next time you type a normal
     character, a `/' character is printed before the character echoes.

     This is a BSD extension, and exists only in BSD systems and the
     GNU system.

 - Macro: tcflag_t ECHOK
     This bit enables special display of the KILL character by moving
     to a new line after echoing the KILL character normally.  The
     behavior of `ECHOKE' (below) is nicer to look at.

     If this bit is not set, the KILL character echoes just as it would
     if it were not the KILL character.  Then it is up to the user to
     remember that the KILL character has erased the preceding input;
     there is no indication of this on the screen.

     This bit only controls the display behavior; the `ICANON' bit by
     itself controls actual recognition of the KILL character and
     erasure of input, without which `ECHOK' is simply irrelevant.

 - Macro: tcflag_t ECHOKE
     This bit is similar to `ECHOK'.  It enables special display of the
     KILL character by erasing on the screen the entire line that has
     been killed.  This is a BSD extension, and exists only in BSD
     systems and the GNU system.

 - Macro: tcflag_t ECHONL
     If this bit is set and the `ICANON' bit is also set, then the
     newline (`'\n'') character is echoed even if the `ECHO' bit is not
     set.

 - Macro: tcflag_t ECHOCTL
     If this bit is set and the `ECHO' bit is also set, echo control
     characters with `^' followed by the corresponding text character.
     Thus, control-A echoes as `^A'.  This is usually the preferred mode
     for interactive input, because echoing a control character back to
     the terminal could have some undesired effect on the terminal.

     This is a BSD extension, and exists only in BSD systems and the
     GNU system.

 - Macro: tcflag_t ISIG
     This bit controls whether the INTR, QUIT, and SUSP characters are
     recognized.  The functions associated with these characters are
     performed if and only if this bit is set.  Being in canonical or
     noncanonical input mode has no affect on the interpretation of
     these characters.

     You should use caution when disabling recognition of these
     characters.  Programs that cannot be interrupted interactively are
     very user-unfriendly.  If you clear this bit, your program should
     provide some alternate interface that allows the user to
     interactively send the signals associated with these characters,
     or to escape from the program.

     *Note Signal Characters::.

 - Macro: tcflag_t IEXTEN
     POSIX.1 gives `IEXTEN' implementation-defined meaning, so you
     cannot rely on this interpretation on all systems.

     On BSD systems and the GNU system, it enables the LNEXT and
     DISCARD characters.  *Note Other Special::.

 - Macro: tcflag_t NOFLSH
     Normally, the INTR, QUIT, and SUSP characters cause input and
     output queues for the terminal to be cleared.  If this bit is set,
     the queues are not cleared.

 - Macro: tcflag_t TOSTOP
     If this bit is set and the system supports job control, then
     `SIGTTOU' signals are generated by background processes that
     attempt to write to the terminal.  *Note Access to the Terminal::.

   The following bits are BSD extensions; they exist only in BSD systems
and the GNU system.

 - Macro: tcflag_t ALTWERASE
     This bit determines how far the WERASE character should erase.  The
     WERASE character erases back to the beginning of a word; the
     question is, where do words begin?

     If this bit is clear, then the beginning of a word is a
     nonwhitespace character following a whitespace character.  If the
     bit is set, then the beginning of a word is an alphanumeric
     character or underscore following a character which is none of
     those.

     *Note Editing Characters::, for more information about the WERASE
     character.

 - Macro: tcflag_t FLUSHO
     This is the bit that toggles when the user types the DISCARD
     character.  While this bit is set, all output is discarded.  *Note
     Other Special::.

 - Macro: tcflag_t NOKERNINFO
     Setting this bit disables handling of the STATUS character.  *Note
     Other Special::.

 - Macro: tcflag_t PENDIN
     If this bit is set, it indicates that there is a line of input that
     needs to be reprinted.  Typing the REPRINT character sets this
     bit; the bit remains set until reprinting is finished.  *Note
     Editing Characters::.


File: libc.info,  Node: Line Speed,  Next: Special Characters,  Prev: Local Modes,  Up: Terminal Modes

Line Speed
----------

   The terminal line speed tells the computer how fast to read and write
data on the terminal.

   If the terminal is connected to a real serial line, the terminal
speed you specify actually controls the line--if it doesn't match the
terminal's own idea of the speed, communication does not work.  Real
serial ports accept only certain standard speeds.  Also, particular
hardware may not support even all the standard speeds.  Specifying a
speed of zero hangs up a dialup connection and turns off modem control
signals.

   If the terminal is not a real serial line (for example, if it is a
network connection), then the line speed won't really affect data
transmission speed, but some programs will use it to determine the
amount of padding needed.  It's best to specify a line speed value that
matches the actual speed of the actual terminal, but you can safely
experiment with different values to vary the amount of padding.

   There are actually two line speeds for each terminal, one for input
and one for output.  You can set them independently, but most often
terminals use the same speed for both directions.

   The speed values are stored in the `struct termios' structure, but
don't try to access them in the `struct termios' structure directly.
Instead, you should use the following functions to read and store them:

 - Function: speed_t cfgetospeed (const struct termios *TERMIOS-P)
     This function returns the output line speed stored in the structure
     `*TERMIOS-P'.

 - Function: speed_t cfgetispeed (const struct termios *TERMIOS-P)
     This function returns the input line speed stored in the structure
     `*TERMIOS-P'.

 - Function: int cfsetospeed (struct termios *TERMIOS-P, speed_t SPEED)
     This function stores SPEED in `*TERMIOS-P' as the output speed.
     The normal return value is 0; a value of -1 indicates an error.
     If SPEED is not a speed, `cfsetospeed' returns -1.

 - Function: int cfsetispeed (struct termios *TERMIOS-P, speed_t SPEED)
     This function stores SPEED in `*TERMIOS-P' as the input speed.
     The normal return value is 0; a value of -1 indicates an error.
     If SPEED is not a speed, `cfsetospeed' returns -1.

 - Function: int cfsetspeed (struct termios *TERMIOS-P, speed_t SPEED)
     This function stores SPEED in `*TERMIOS-P' as both the input and
     output speeds.  The normal return value is 0; a value of -1
     indicates an error.  If SPEED is not a speed, `cfsetspeed' returns
     -1.  This function is an extension in 4.4 BSD.

 - Data Type: speed_t
     The `speed_t' type is an unsigned integer data type used to
     represent line speeds.

   The functions `cfsetospeed' and `cfsetispeed' report errors only for
speed values that the system simply cannot handle.  If you specify a
speed value that is basically acceptable, then those functions will
succeed.  But they do not check that a particular hardware device can
actually support the specified speeds--in fact, they don't know which
device you plan to set the speed for.  If you use `tcsetattr' to set
the speed of a particular device to a value that it cannot handle,
`tcsetattr' returns -1.

   *Portability note:* In the GNU library, the functions above accept
speeds measured in bits per second as input, and return speed values
measured in bits per second.  Other libraries require speeds to be
indicated by special codes.  For POSIX.1 portability, you must use one
of the following symbols to represent the speed; their precise numeric
values are system-dependent, but each name has a fixed meaning: `B110'
stands for 110 bps, `B300' for 300 bps, and so on.  There is no
portable way to represent any speed but these, but these are the only
speeds that typical serial lines can support.

     B0  B50  B75  B110  B134  B150  B200
     B300  B600  B1200  B1800  B2400  B4800
     B9600  B19200  B38400  B57600  B115200
     B230400  B460800

   BSD defines two additional speed symbols as aliases: `EXTA' is an
alias for `B19200' and `EXTB' is an alias for `B38400'.  These aliases
are obsolete.


File: libc.info,  Node: Special Characters,  Next: Noncanonical Input,  Prev: Line Speed,  Up: Terminal Modes

Special Characters
------------------

   In canonical input, the terminal driver recognizes a number of
special characters which perform various control functions.  These
include the ERASE character (usually <DEL>) for editing input, and
other editing characters.  The INTR character (normally `C-c') for
sending a `SIGINT' signal, and other signal-raising characters, may be
available in either canonical or noncanonical input mode.  All these
characters are described in this section.

   The particular characters used are specified in the `c_cc' member of
the `struct termios' structure.  This member is an array; each element
specifies the character for a particular role.  Each element has a
symbolic constant that stands for the index of that element--for
example, `VINTR' is the index of the element that specifies the INTR
character, so storing `'='' in `TERMIOS.c_cc[VINTR]' specifies `=' as
the INTR character.

   On some systems, you can disable a particular special character
function by specifying the value `_POSIX_VDISABLE' for that role.  This
value is unequal to any possible character code.  *Note Options for
Files::, for more information about how to tell whether the operating
system you are using supports `_POSIX_VDISABLE'.

* Menu:

* Editing Characters::          Special characters that terminate lines and
                                  delete text, and other editing functions.
* Signal Characters::           Special characters that send or raise signals
                                  to or for certain classes of processes.
* Start/Stop Characters::       Special characters that suspend or resume
                                  suspended output.
* Other Special::		Other special characters for BSD systems:
				  they can discard output, and print status.

