Documentation for /proc/sys/kernel/*	kernel version 2.2.10
	(c) 1998, 1999,  Rik van Riel <riel@nl.linux.org>

For general info and legal blurb, please look in README.

==============================================================

This file contains documentation for the sysctl files in
/proc/sys/kernel/ and is valid for Linux kernel version 2.2.

The files in this directory can be used to tune and monitor
miscellaneous and general things in the operation of the Linux
kernel. Since some of the files _can_ be used to screw up your
system, it is advisable to read both documentation and source
before actually making adjustments.

Currently, these files might (depending on your configuration)
show up in /proc/sys/kernel:
- acct
- ctrl-alt-del
- dentry-state
- domainname
- hostname
- htab-reclaim                [ PPC only ]
- java-appletviewer           [ binfmt_java, obsolete ]
- java-interpreter            [ binfmt_java, obsolete ]
- l2cr                        [ PPC only ]
- modprobe                    ==> Documentation/kmod.txt
- osrelease
- ostype
- panic
- powersave-nap               [ PPC only ]
- printk
- real-root-dev               ==> Documentation/initrd.txt
- reboot-cmd                  [ SPARC only ]
- rtsig-nr
- rtsig-max
- sg-big-buff                 [ generic SCSI device (sg) ]
- shmmax                      [ sysv ipc ]
- version
- zero-paged                  [ PPC only ]

==============================================================

acct:

highwater lowwater frequency

If BSD-style process accounting is enabled these values control
its behaviour. If free space on filesystem where the log lives
goes below <lowwater>% accounting suspends. If free space gets
above <highwater>% accounting resumes. <Frequency> determines
how often do we check the amount of free space (value is in
seconds). Default:
4 2 30
That is, suspend accounting if there left <= 2% free; resume it
if we got >=4%; consider information about amount of free space
valid for 30 seconds.

==============================================================

ctrl-alt-del:

When the value in this file is 0, ctrl-alt-del is trapped and
sent to the init(1) program to handle a graceful restart.
When, however, the value is > 0, Linux's reaction to a Vulcan
Nerve Pinch (tm) will be an immediate reboot, without even
syncing its dirty buffers.

Note: when a program (like dosemu) has the keyboard in 'raw'
mode, the ctrl-alt-del is intercepted by the program before it
ever reaches the kernel tty layer, and it's up to the program
to decide what to do with it.

==============================================================

domainname & hostname:

These files can be used to set the NIS/YP domainname and the
hostname of your box in exactly the same way as the commands
domainname and hostname, i.e.:
# echo "darkstar" > /proc/sys/kernel/hostname
# echo "mydomain" > /proc/sys/kernel/domainname
has the same effect as
# hostname "darkstar" > /proc/sys/kernel/hostname
# domainname "mydomain" > /proc/sys/kernel/domainname

Note, however, that the classic darkstar.frop.org has the
hostname "darkstar" and DNS (Internet Domain Name Server)
domainname "frop.org", not to be confused with the NIS (Network
Information Service) or YP (Yellow Pages) domainname. These two
domain names are in general different. For a detailed discussion
see the hostname(1) man page.

==============================================================

htab-reclaim: (PPC only)

Setting this to a non-zero value, the PowerPC htab
(see Documentation/powerpc/ppc_htab.txt) is pruned
each time the system hits the idle loop.
 
==============================================================

l2cr: (PPC only)

This flag controls the L2 cache of G3 processor boards. If
0, the cache is disabled. Enabled if nonzero.

==============================================================

osrelease, ostype & version:

# cat osrelease
2.1.88
# cat ostype
Linux
# cat version
#5 Wed Feb 25 21:49:24 MET 1998

The files osrelease and ostype should be clear enough. Version
needs a little more clarification however. The '#5' means that
this is the fifth kernel built from this source base and the
date behind it indicates the time the kernel was built.
The only way to tune these values is to rebuild the kernel :-)

==============================================================

panic:

The value in this file represents the number of seconds the
kernel waits before rebooting on a panic. When you use the
software watchdog, the recommended setting is 60.

==============================================================

powersave-nap: (PPC only)

If set, Linux-PPC will use the 'nap' mode of powersaving,
otherwise the 'doze' mode will be used.

==============================================================

printk:

The four values in printk denote: console_loglevel,
default_message_loglevel, minimum_console_level and
default_console_loglevel respectively.

These values influence printk() behavior when printing or
logging error messages. See 'man 2 syslog' for more info on
the different loglevels.

- console_loglevel: messages with a higher priority than
  this will be printed to the console
- default_message_level: messages without an explicit priority
  will be printed with this priority
- minimum_console_loglevel: minimum (highest) value to which
  console_loglevel can be set
- default_console_loglevel: default value for console_loglevel

Note: a quick look in linux/kernel/printk.c will reveal that
these variables aren't put inside a structure, so their order
in-core isn't formally guaranteed and garbage values _might_
occur when the compiler changes. (???)

==============================================================

reboot-cmd: (Sparc only)

??? This seems to be a way to give an argument to the Sparc
ROM/Flash boot loader. Maybe to tell it what to do after
rebooting. ???

==============================================================

rtsig-max & rtsig-nr:

The file rtsig-max can be used to tune the maximum number
of POSIX realtime (queued) signals that can be outstanding
in the system.

Rtsig-nr shows the number of RT signals currently queued.

==============================================================

sg-big-buff:

This file shows the size of the generic SCSI (sg) buffer.
You can't tune it just yet, but you could change it on
compile time by editing include/scsi/sg.h and changing
the value of SG_BIG_BUFF.

There shouldn't be any reason to change this value. If
you can come up with one, you probably know what you
are doing anyway :)

==============================================================

shmmax: 

This value can be used to query and set the run time limit
on the maximum shared memory segment size that can be created.
Shared memory segments up to 1Gb are now supported in the 
kernel.  This value defaults to SHMMAX.

==============================================================

zero-paged: (PPC only)

When enabled (non-zero), Linux-PPC will pre-zero pages in
the idle loop, possibly speeding up get_free_pages. Since
this only affects what the idle loop is doing, you should
enable this and see if anything changes.
