
Is your SMP system locking up unpredictably? No keyboard activity, just
a frustrating complete hard lockup? Do you want to help us debugging
such lockups? If all yes then this document is definitely for you.

on Intel SMP hardware there is a feature that enables us to generate
'watchdog NMI interrupts'. (NMI: Non Maskable Interrupt - these get
executed even if the system is otherwise locked up hard) This can be
used to debug hard kernel lockups. By executing periodic NMI interrupts,
the kernel can monitor wether any CPU has locked up, and print out
debugging messages if so.  You can enable/disable the NMI watchdog at boot
time with the 'nmi_watchdog=1' boot parameter. Eg. the relevant
lilo.conf entry:

        append="nmi_watchdog=1"

A 'lockup' is the following scenario: if any CPU in the system does not
execute the period local timer interrupt for more than 5 seconds, then
the NMI handler generates an oops and kills the process. This
'controlled crash' (and the resulting kernel messages) can be used to
debug the lockup. Thus whenever the lockup happens, wait 5 seconds and
the oops will show up automatically. If the kernel produces no messages
then the system has crashed so hard (eg. hardware-wise) that either it
cannot even accept NMI interrupts, or the crash has made the kernel
unable to print messages.

You can find NMI watchdog patch against Linux 2.2.x at 
http://people.redhat.com/mingo/NMI-watchdog-patches/


[ feel free to send bug reports, suggestions and patches to
  Ingo Molnar <mingo@redhat.com> or the Linux SMP mailing
  list at <linux-smp@vger.kernel.org> ]

