This driver is for Compaq's SMART Array Controllers.

Supported Cards:
----------------

This driver is known to work with the following cards:

	* SA 5300
	* SA 5i
	* SA 532

If notes are not already created in the /dev/cciss directory

# mkdev.cciss [ctlrs]

Where ctlrs is the number of controllers you have (defaults to 1 if not
specified).

Device Naming:
--------------

You need some entries in /dev for the cciss device.  The mkdev.cciss script
can make device nodes for you automatically.  Currently the device setup
is as follows:

Major numbers:
	104	cciss0	
	105	cciss1	
	106	cciss2 
	etc...

Minor numbers:
        b7 b6 b5 b4 b3 b2 b1 b0
        |----+----| |----+----|
             |           |
             |           +-------- Partition ID (0=wholedev, 1-15 partition)
             |
             +-------------------- Logical Volume number

The suggested device naming scheme is:
/dev/cciss/c0d0			Controller 0, disk 0, whole device
/dev/cciss/c0d0p1		Controller 0, disk 0, partition 1
/dev/cciss/c0d0p2		Controller 0, disk 0, partition 2
/dev/cciss/c0d0p3		Controller 0, disk 0, partition 3

/dev/cciss/c1d1			Controller 1, disk 1, whole device
/dev/cciss/c1d1p1		Controller 1, disk 1, partition 1
/dev/cciss/c1d1p2		Controller 1, disk 1, partition 2
/dev/cciss/c1d1p3		Controller 1, disk 1, partition 3
