; This file is executed after the print is finished
; Depending on your settings you can:
; - retract filament a bit more, so it doesn't ooze
; - turn the heated bed/extruder off
; - go to waiting position
