;  Commands in this file are send before the generated G-Code is send
; Use it to initialize your printer position and extruder temperature
;M104 S180 ; Set Extruder temperature
;M140 S55 ; Set heated bed temperature
;M109 ; Wait for temperature to reach target temp
;M28 X0 Y0 Z0 ; Initialize coordinate system
;If your extruder drolls, refill it with plastic before you start the print
