--- a/drivers/leds/Kconfig
+++ b/drivers/leds/Kconfig
@@ -77,6 +77,12 @@ config LEDS_WRAP
 	help
 	  This option enables support for the PCEngines WRAP programmable LEDs.
 
+config LEDS_ALIX
+	tristate "LED Support for the ALIX 2/3 boards"
+	depends on LEDS_CLASS
+	help
+	  This option enables support for the three LEDs on the PCEngines ALIX 2/3 boards.
+
 config LEDS_H1940
 	tristate "LED Support for iPAQ H1940 device"
 	depends on LEDS_CLASS && ARCH_H1940
--- a/drivers/leds/Makefile
+++ b/drivers/leds/Makefile
@@ -13,6 +13,7 @@ obj-$(CONFIG_LEDS_S3C24XX)		+= leds-s3c2
 obj-$(CONFIG_LEDS_AMS_DELTA)		+= leds-ams-delta.o
 obj-$(CONFIG_LEDS_NET48XX)		+= leds-net48xx.o
 obj-$(CONFIG_LEDS_WRAP)			+= leds-wrap.o
+obj-$(CONFIG_LEDS_ALIX)			+= leds-alix.o
 obj-$(CONFIG_LEDS_H1940)		+= leds-h1940.o
 obj-$(CONFIG_LEDS_COBALT_QUBE)		+= leds-cobalt-qube.o
 obj-$(CONFIG_LEDS_COBALT_RAQ)		+= leds-cobalt-raq.o
