--- a/drivers/net/phy/mdio_bus.c
+++ b/drivers/net/phy/mdio_bus.c
@@ -135,6 +135,9 @@ static int mdio_bus_match(struct device 
 	struct phy_device *phydev = to_phy_device(dev);
 	struct phy_driver *phydrv = to_phy_driver(drv);
 
+	if (phydrv->detect)
+		return (phydrv->detect(phydev->bus, phydev->addr));
+
 	return ((phydrv->phy_id & phydrv->phy_id_mask) ==
 		(phydev->phy_id & phydrv->phy_id_mask));
 }
--- a/include/linux/phy.h
+++ b/include/linux/phy.h
@@ -339,6 +339,11 @@ struct phy_driver {
 	u32 features;
 	u32 flags;
 
+	/* Called during discovery to test if the
+	 * device can attach to the bus, even if
+	 * phy id and mask do not match */
+	bool (*detect)(struct mii_bus *bus, int addr);
+
 	/*
 	 * Called to initialize the PHY,
 	 * including after a reset
