diff -urN compat-wireless-2008-08-06/config.mk compat-wireless-2008-08-06.new/config.mk
--- compat-wireless-2008-08-06/config.mk	2008-07-18 06:11:03.000000000 +0200
+++ compat-wireless-2008-08-06.new/config.mk	2008-08-20 17:30:13.000000000 +0200
@@ -72,70 +72,6 @@
 CONFIG_ATH5K=m
 CONFIG_ATH5K_DEBUG=n
 
-# Required for older kernels which still use this flag.
-CONFIG_IWLWIFI=m
-
-CONFIG_IWLCORE=m
-CONFIG_IWL3945=m
-CONFIG_IWL4965=m
-CONFIG_IWL4965_HT=y
-CONFIG_B43=m
-# B43 uses PCMCIA only for Compact Flash. The Cardbus cards uses PCI
-# Example, bcm4318:
-# http://www.multicap.biz/wireless-lan/indoor-wlan-hardware/sdc-cf10g-80211g-compact-flash-module
-CONFIG_B43_PCMCIA=y
-CONFIG_B43_DMA=y
-CONFIG_B43_PIO=y
-# B43_PIO selects SSB_BLOCKIO
-CONFIG_SSB_BLOCKIO=y
-CONFIG_B43_DMA_AND_PIO_MODE=y
-CONFIG_B43_PCI_AUTOSELECT=y
-CONFIG_B43_PCICORE_AUTOSELECT=y
-#CONFIG_B43_RFKILL=n
-CONFIG_B43_LEDS=y
-# CONFIG_B43_DEBUG is not set
-
-CONFIG_B43LEGACY=m
-CONFIG_B43LEGACY_PCI_AUTOSELECT=y
-CONFIG_B43LEGACY_PCICORE_AUTOSELECT=y
-CONFIG_B43LEGACY_DMA=y
-CONFIG_B43LEGACY_PIO=y
-CONFIG_B43LEGACY_DMA_AND_PIO_MODE=y
-
-# The Intel ipws
-CONFIG_IPW2100=m
-CONFIG_IPW2100_MONITOR=y
-CONFIG_IPW2200=m
-CONFIG_IPW2200_MONITOR=y
-CONFIG_IPW2200_RADIOTAP=y
-CONFIG_IPW2200_PROMISCUOUS=y
-# The above enables use a second interface prefixed 'rtap'.
-#           Example usage:
-#
-# % modprobe ipw2200 rtap_iface=1
-# % ifconfig rtap0 up
-# % tethereal -i rtap0
-#
-# If you do not specify 'rtap_iface=1' as a module parameter then
-# the rtap interface will not be created and you will need to turn
-# it on via sysfs:
-#
-# % echo 1 > /sys/bus/pci/drivers/ipw2200/*/rtap_iface
-CONFIG_IPW2200_QOS=y
-
-NEED_IEEE80211=y
-
-CONFIG_P54_PCI=m
-
-CONFIG_SSB_PCIHOST_POSSIBLE=y
-CONFIG_SSB_PCIHOST=y
-CONFIG_SSB_DRIVER_PCICORE_POSSIBLE=y
-CONFIG_SSB_DRIVER_PCICORE=y
-CONFIG_SSB_B43_PCI_BRIDGE=y
-
-CONFIG_RTL8180=m
-CONFIG_ADM8211=m
-
 CONFIG_RT2X00_LIB_PCI=m
 CONFIG_RT2400PCI=m
 CONFIG_RT2500PCI=m
@@ -159,32 +95,6 @@
 ifneq ($(CONFIG_USB),)
 CONFIG_ZD1211RW=m
 
-# support for USB Wireless devices using Atmel at76c503,
-# at76c505 or at76c505a chips.
-CONFIG_USB_ATMEL=m
-
-# Stuff here things which depend on kernel versions for USB
-ifeq ($(shell test -e $(KLIB_BUILD)/Makefile && echo yes),yes)
-KERNEL_SUBLEVEL = $(shell $(MAKE) -C $(KLIB_BUILD) kernelversion | sed -n 's/^2\.6\.\([0-9]\+\).*/\1/p')
-ifeq ($(shell test $(KERNEL_SUBLEVEL) -gt 21 && echo yes),yes)
-
-# Sorry, rndis_wlan uses cancel_work_sync which is new and can't be done in compat...
-
-# Wireless RNDIS USB support (RTL8185 802.11g) A-Link WL54PC
-# All of these devices are based on Broadcom 4320 chip which
-# is only wireless RNDIS chip known to date.
-# Note: this depends on CONFIG_USB_NET_RNDIS_HOST and CONFIG_USB_NET_CDCETHER
-# it also requires new RNDIS_HOST and CDC_ETHER modules which we add
-CONFIG_USB_NET_RNDIS_HOST=m
-CONFIG_USB_NET_RNDIS_WLAN=m
-CONFIG_USB_NET_CDCETHER=m
-
-endif
-endif
-
-CONFIG_P54_USB=m
-CONFIG_RTL8187=m
-
 # RT2500USB does not require firmware
 CONFIG_RT2500USB=m
 CONFIG_RT2X00_LIB_USB=m
@@ -209,39 +119,6 @@
 CONFIG_RT2X00_LIB_FIRMWARE=y
 endif
 
-# p54
-CONFIG_P54_COMMON=m
-
-# Sonics Silicon Backplane
-CONFIG_SSB_POSSIBLE=y
-CONFIG_SSB=m
-CONFIG_SSB_SPROM=y
-
-ifneq ($(CONFIG_PCMCIA),)
-CONFIG_SSB_PCMCIAHOST=y
-endif
-
-# These two are for mips
-CONFIG_SSB_DRIVER_MIPS=n
-CONFIG_SSB_PCICORE_HOSTMODE=n
-# CONFIG_SSB_DEBUG is not set
-# CONFIG_SSB_DRIVER_EXTIF=y
-
-ifneq ($(CONFIG_USB),)
-CONFIG_LIBERTAS_USB=m
-NEED_LIBERTAS=y
-endif
-ifneq ($(CONFIG_PCMCIA),)
-CONFIG_LIBERTAS_CS=m
-NEED_LIBERTAS=y
-endif
-ifeq ($(NEED_LIBERTAS),y)
-CONFIG_LIBERTAS=m
-# Libertas uses the old stack but not fully, it will soon 
-# be cleaned.
-NEED_IEEE80211=y
-endif
-
 ifeq ($(NEED_IEEE80211),y)
 # Old ieee80211 "stack"
 # Note: old softmac is scheduled for removal so we
