--- a/drivers/net/phy/phy.c
+++ b/drivers/net/phy/phy.c
@@ -344,6 +344,50 @@ int phy_ethtool_gset(struct phy_device *
 }
 EXPORT_SYMBOL(phy_ethtool_gset);
 
+int phy_ethtool_ioctl(struct phy_device *phydev, void *useraddr)
+{
+	u32 cmd;
+	int tmp;
+	struct ethtool_cmd ecmd = { ETHTOOL_GSET };
+	struct ethtool_value edata = { ETHTOOL_GLINK };
+
+	if (get_user(cmd, (u32 *) useraddr))
+		return -EFAULT;
+
+	switch (cmd) {
+	case ETHTOOL_GSET:
+		phy_ethtool_gset(phydev, &ecmd);
+		if (copy_to_user(useraddr, &ecmd, sizeof(ecmd)))
+			return -EFAULT;
+		return 0;
+	
+	case ETHTOOL_SSET:
+		if (copy_from_user(&ecmd, useraddr, sizeof(ecmd)))
+			return -EFAULT;
+		return phy_ethtool_sset(phydev, &ecmd);
+
+	case ETHTOOL_NWAY_RST:
+		/* if autoneg is off, it's an error */
+		tmp = phy_read(phydev, MII_BMCR);
+		if (tmp & BMCR_ANENABLE) {
+			tmp |= (BMCR_ANRESTART);
+			phy_write(phydev, MII_BMCR, tmp);
+			return 0;
+		}	
+		return -EINVAL;
+
+	case ETHTOOL_GLINK:
+		edata.data = (phy_read(phydev,
+				MII_BMSR) & BMSR_LSTATUS) ? 1 : 0;
+		if (copy_to_user(useraddr, &edata, sizeof(edata)))
+			return -EFAULT;
+		return 0;
+	}
+
+	return -EOPNOTSUPP;
+}
+EXPORT_SYMBOL(phy_ethtool_ioctl);
+
 /**
  * phy_mii_ioctl - generic PHY MII ioctl interface
  * @phydev: the phy_device struct
--- a/include/linux/phy.h
+++ b/include/linux/phy.h
@@ -393,6 +393,7 @@ void phy_start_machine(struct phy_device
 void phy_stop_machine(struct phy_device *phydev);
 int phy_ethtool_sset(struct phy_device *phydev, struct ethtool_cmd *cmd);
 int phy_ethtool_gset(struct phy_device *phydev, struct ethtool_cmd *cmd);
+int phy_ethtool_ioctl(struct phy_device *phydev, void *useraddr);
 int phy_mii_ioctl(struct phy_device *phydev,
 		struct mii_ioctl_data *mii_data, int cmd);
 int phy_start_interrupts(struct phy_device *phydev);
