--- a/drivers/mtd/maps/Kconfig
+++ b/drivers/mtd/maps/Kconfig
@@ -337,6 +337,12 @@ config MTD_CFI_FLAGADM
 	  Mapping for the Flaga digital module. If you don't have one, ignore
 	  this setting.
 
+config MTD_BCM47XX
+	tristate "BCM47xx flash device"
+	depends on MIPS && MTD_CFI && BCM47XX
+	help
+	  Support for the flash chips on the BCM947xx board.
+
 config MTD_WALNUT
 	tristate "Flash device mapped on IBM 405GP Walnut"
 	depends on MTD_JEDECPROBE && WALNUT && !PPC_MERGE
--- a/drivers/mtd/maps/Makefile
+++ b/drivers/mtd/maps/Makefile
@@ -31,6 +31,7 @@ obj-$(CONFIG_MTD_PMC_MSP_RAMROOT)+= pmcm
 obj-$(CONFIG_MTD_PCMCIA)	+= pcmciamtd.o
 obj-$(CONFIG_MTD_RPXLITE)	+= rpxlite.o
 obj-$(CONFIG_MTD_TQM8XXL)	+= tqm8xxl.o
+obj-$(CONFIG_MTD_BCM47XX)	+= bcm47xx-flash.o
 obj-$(CONFIG_MTD_SA1100)	+= sa1100-flash.o
 obj-$(CONFIG_MTD_IPAQ)		+= ipaq-flash.o
 obj-$(CONFIG_MTD_SBC_GXX)	+= sbc_gxx.o
