--- a/drivers/ssb/main.c
+++ b/drivers/ssb/main.c
@@ -1173,7 +1173,9 @@ static int __init ssb_modinit(void)
 /* ssb must be initialized after PCI but before the ssb drivers.
  * That means we must use some initcall between subsys_initcall
  * and device_initcall. */
-fs_initcall(ssb_modinit);
+//FIXME on embedded we need to be early to make sure we can register
+//      a new PCI bus, if needed.
+subsys_initcall(ssb_modinit);
 
 static void __exit ssb_modexit(void)
 {
