--- a/networking/udhcp/dhcpc.c
+++ b/networking/udhcp/dhcpc.c
@@ -352,7 +352,7 @@
 
 			switch (state) {
 			case INIT_SELECTING:
-				if (packet_num < discover_retries) {
+				if (!discover_retries || packet_num < discover_retries) {
 					if (packet_num == 0)
 						xid = random_xid();
 
@@ -382,7 +382,7 @@
 				continue;
 			case RENEW_REQUESTED:
 			case REQUESTING:
-				if (packet_num < discover_retries) {
+				if (!discover_retries || packet_num < discover_retries) {
 					/* send request packet */
 					if (state == RENEW_REQUESTED) /* unicast */
 						send_renew(xid, server_addr, requested_ip);
