--- a/drivers/spi/Kconfig
+++ b/drivers/spi/Kconfig
@@ -296,6 +296,11 @@ config SPI_TLE62X0
 	  sysfs interface, with each line presented as a kind of GPIO
 	  exposing both switch control and diagnostic feedback.
 
+config SPI_VSC7385
+	tristate "Vitesse VSC7385 ethernet switch driver"
+	help
+	  SPI driver for the Vitesse VSC7385 ethernet switch.
+
 #
 # Add new SPI protocol masters in alphabetical order above this line
 #
--- a/drivers/spi/Makefile
+++ b/drivers/spi/Makefile
@@ -40,6 +40,7 @@ obj-$(CONFIG_SPI_STMP3XXX)		+= spi_stmp.
 
 # SPI protocol drivers (device/link on bus)
 obj-$(CONFIG_SPI_SPIDEV)	+= spidev.o
+obj-$(CONFIG_SPI_VSC7385)	+= spi_vsc7385.o
 obj-$(CONFIG_SPI_TLE62X0)	+= tle62x0.o
 # 	... add above this line ...
 
