--- a/arch/mips/lantiq/xway/Kconfig
+++ b/arch/mips/lantiq/xway/Kconfig
@@ -6,6 +6,10 @@
 	bool "Easy50712 - Danube"
 	default y
 
+config LANTIQ_MACH_ARV45XX
+	bool "ARV45XX"
+	default y
+
 endmenu
 
 endif
--- a/arch/mips/lantiq/xway/Makefile
+++ b/arch/mips/lantiq/xway/Makefile
@@ -5,3 +5,4 @@
 
 obj-$(CONFIG_LANTIQ_MACH_EASY50712) += mach-easy50712.o
 obj-$(CONFIG_LANTIQ_MACH_EASY50601) += mach-easy50601.o
+obj-$(CONFIG_LANTIQ_MACH_ARV45XX) += mach-arv45xx.o
--- /dev/null
+++ b/arch/mips/lantiq/xway/mach-arv45xx.c
@@ -0,0 +1,504 @@
+/*
+ *  This program is free software; you can redistribute it and/or modify it
+ *  under the terms of the GNU General Public License version 2 as published
+ *  by the Free Software Foundation.
+ *
+ *  Copyright (C) 2010 John Crispin <blogic@openwrt.org>
+ */
+
+#include <linux/init.h>
+#include <linux/platform_device.h>
+#include <linux/leds.h>
+#include <linux/gpio.h>
+#include <linux/gpio_buttons.h>
+#include <linux/mtd/mtd.h>
+#include <linux/mtd/partitions.h>
+#include <linux/mtd/physmap.h>
+#include <linux/input.h>
+#include <linux/etherdevice.h>
+//#include <linux/ath5k_platform.h>
+#include <linux/pci.h>
+
+#include <lantiq_soc.h>
+#include <lantiq_platform.h>
+
+#include "../machtypes.h"
+#include "devices.h"
+#include "dev-leds-gpio.h"
+#include "dev-dwc_otg.h"
+
+#ifdef CONFIG_MTD_PARTITIONS
+static struct mtd_partition arv4510_partitions[] =
+{
+	{
+		.name	= "uboot",
+		.offset	= 0x0,
+		.size	= 0x20000,
+	},
+	{
+		.name	= "uboot_env",
+		.offset	= 0x20000,
+		.size	= 0x120000,
+	},
+	{
+		.name	= "linux",
+		.offset	= 0x40000,
+		.size	= 0xfa0000,
+	},
+	{
+		.name	= "board_config",
+		.offset	= 0xfe0000,
+		.size	= 0x20000,
+	},
+};
+
+static struct mtd_partition arv45xx_partitions[] =
+{
+	{
+		.name	= "uboot",
+		.offset	= 0x0,
+		.size	= 0x20000,
+	},
+	{
+		.name	= "uboot_env",
+		.offset	= 0x20000,
+		.size	= 0x10000,
+	},
+	{
+		.name	= "linux",
+		.offset	= 0x30000,
+		.size	= 0x3c0000,
+	},
+	{
+		.name	= "board_config",
+		.offset	= 0x3f0000,
+		.size	= 0x10000,
+	},
+};
+
+static struct mtd_partition arv75xx_partitions[] =
+{
+	{
+		.name	= "uboot",
+		.offset	= 0x0,
+		.size	= 0x10000,
+	},
+	{
+		.name	= "uboot_env",
+		.offset	= 0x10000,
+		.size	= 0x10000,
+	},
+	{
+		.name	= "linux",
+		.offset	= 0x20000,
+		.size	= 0x7d0000,
+	},
+	{
+		.name	= "board_config",
+		.offset	= 0x7f0000,
+		.size	= 0x10000,
+	},
+};
+
+#endif
+
+static struct physmap_flash_data arv4510_flash_data = {
+#ifdef CONFIG_MTD_PARTITIONS
+	.nr_parts	= ARRAY_SIZE(arv4510_partitions),
+	.parts		= arv4510_partitions,
+#endif
+};
+
+static struct physmap_flash_data arv45xx_flash_data = {
+#ifdef CONFIG_MTD_PARTITIONS
+	.nr_parts	= ARRAY_SIZE(arv45xx_partitions),
+	.parts		= arv45xx_partitions,
+#endif
+};
+
+static struct physmap_flash_data arv75xx_flash_data = {
+#ifdef CONFIG_MTD_PARTITIONS
+	.nr_parts	= ARRAY_SIZE(arv75xx_partitions),
+	.parts		= arv75xx_partitions,
+#endif
+};
+
+static struct ltq_pci_data ltq_pci_data = {
+	.clock  = PCI_CLOCK_EXT,
+	.gpio   = PCI_GNT1 | PCI_REQ1,
+	.irq    = {
+		[14] = INT_NUM_IM0_IRL0 + 22,
+	},
+};
+
+static struct ltq_eth_data ltq_eth_data = {
+	.mii_mode	= PHY_INTERFACE_MODE_RMII,
+};
+
+static struct gpio_led
+arv4510pw_leds_gpio[] __initdata = {
+	{ .name = "soc:green:foo", .gpio = 4, .active_low = 1, },
+};
+
+static struct gpio_led
+arv4518pw_leds_gpio[] __initdata = {
+	{ .name = "soc:green:power", .gpio = 3, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:green:adsl", .gpio = 4, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:green:internet", .gpio = 5, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:green:wlan", .gpio = 6, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:yellow:wps", .gpio = 7, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:red:fail", .gpio = 8, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:green:usb", .gpio = 19, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:green:voip", .gpio = 72, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:green:fxs1", .gpio = 73, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:green:fxs2", .gpio = 74, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:green:fxo", .gpio = 75, .active_low = 1, .default_trigger = "default-on" },
+};
+
+static struct gpio_button
+arv4518pw_gpio_buttons[] __initdata = {
+	{ .desc = "wlan", .type = EV_KEY, .code = BTN_0, .threshold = 3, .gpio = 28, .active_low = 1, },
+	{ .desc = "wps", .type = EV_KEY, .code = BTN_1, .threshold = 3, .gpio = 29, .active_low = 1, },
+	{ .desc = "reset", .type = EV_KEY, .code = BTN_2, .threshold = 3, .gpio = 30, .active_low = 1, },
+};
+
+static struct gpio_led
+arv4520pw_leds_gpio[] __initdata = {
+	{ .name = "soc:blue:power", .gpio = 3, .active_low = 1, },
+	{ .name = "soc:blue:adsl", .gpio = 4, .active_low = 1, },
+	{ .name = "soc:blue:internet", .gpio = 5, .active_low = 1, },
+	{ .name = "soc:red:power", .gpio = 6, .active_low = 1, },
+	{ .name = "soc:yellow:wps", .gpio = 7, .active_low = 1, },
+	{ .name = "soc:red:wps", .gpio = 9, .active_low = 1, },
+	{ .name = "soc:blue:voip", .gpio = 72, .active_low = 1, },
+	{ .name = "soc:blue:fxs1", .gpio = 73, .active_low = 1, },
+	{ .name = "soc:blue:fxs2", .gpio = 74, .active_low = 1, },
+	{ .name = "soc:blue:fxo", .gpio = 75, .active_low = 1, },
+	{ .name = "soc:blue:voice", .gpio = 76, .active_low = 1, },
+	{ .name = "soc:blue:usb", .gpio = 77, .active_low = 1, },
+	{ .name = "soc:blue:wlan", .gpio = 78, .active_low = 1, },
+};
+
+static struct gpio_led
+arv452cpw_leds_gpio[] __initdata = {
+	{ .name = "soc:blue:power", .gpio = 3, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:blue:adsl", .gpio = 4, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:blue:isdn", .gpio = 5, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:red:power", .gpio = 6, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:yellow:wps", .gpio = 7, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:red:wps", .gpio = 9, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:blue:fxs1", .gpio = 72, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:blue:fxs2", .gpio = 73, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:blue:wps", .gpio = 74, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:blue:fxo", .gpio = 75, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:blue:voice", .gpio = 76, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:blue:usb", .gpio = 77, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:blue:wlan", .gpio = 78, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:blue:internet", .gpio = 80, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:red:internet", .gpio = 81, .active_low = 1, .default_trigger = "default-on" },
+};
+
+static struct gpio_led
+arv4525pw_leds_gpio[] __initdata = {
+	{ .name = "soc:green:festnetz", .gpio = 4, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:green:internet", .gpio = 5, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:green:dsl", .gpio = 6, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:green:wlan", .gpio = 8, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:green:online", .gpio = 9, .active_low = 1, .default_trigger = "default-on" },
+};
+
+static struct gpio_led
+arv752dpw22_leds_gpio[] __initdata = {
+	{ .name = "soc:blue:power", .gpio = 3, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:red:internet", .gpio = 5, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:red:power", .gpio = 6, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:red:wps", .gpio = 8, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:red:fxo", .gpio = 75, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:red:voice", .gpio = 76, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:green:usb", .gpio = 77, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:green:wlan", .gpio = 78, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:green:wlan1", .gpio = 79, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:blue:wlan", .gpio = 80, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:blue:wlan1", .gpio = 81, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:green:eth1", .gpio = 83, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:green:eth2", .gpio = 84, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:green:eth3", .gpio = 85, .active_low = 1, .default_trigger = "default-on" },
+	{ .name = "soc:green:eth4", .gpio = 86, .active_low = 1, .default_trigger = "default-on", },
+};
+
+static struct gpio_button
+arv752dpw22_gpio_buttons[] __initdata = {
+	{ .desc = "btn0", .type = EV_KEY, .code = BTN_0, .threshold = 3, .gpio = 12, .active_low = 1, },
+	{ .desc = "btn1", .type = EV_KEY, .code = BTN_1, .threshold = 3, .gpio = 13, .active_low = 1, },
+	{ .desc = "btn2", .type = EV_KEY, .code = BTN_2, .threshold = 3, .gpio = 28, .active_low = 1, },
+};
+
+static struct gpio_led
+arv7518pw_leds_gpio[] __initdata = {
+	{ .name = "soc:green:power", .gpio = 2, .active_low = 1, },
+	{ .name = "soc:green:adsl", .gpio = 4, .active_low = 1, },
+	{ .name = "soc:green:internet", .gpio = 5, .active_low = 1, },
+	{ .name = "soc:green:wlan", .gpio = 6, .active_low = 1, },
+	{ .name = "soc:red:internet", .gpio = 8, .active_low = 1, },
+	{ .name = "soc:green:usb", .gpio = 19, .active_low = 1, },
+};
+
+static struct gpio_button
+arv7518pw_gpio_buttons[] __initdata = {
+	{ .desc = "reset", .type = EV_KEY, .code = BTN_0, .threshold = 3, .gpio = 23, .active_low = 1, },
+	{ .desc = "wlan", .type = EV_KEY, .code = BTN_1, .threshold = 3, .gpio = 25, .active_low = 1, },
+};
+
+static void
+arv45xx_register_ethernet(void)
+{
+#define ARV45XX_BRN_MAC			0x3f0016
+	memcpy_fromio(&ltq_eth_data.mac.sa_data,
+		(void *)KSEG1ADDR(LTQ_FLASH_START + ARV45XX_BRN_MAC), 6);
+	ltq_register_etop(&ltq_eth_data);
+}
+
+static void
+arv75xx_register_ethernet(void)
+{
+#define ARV75XX_BRN_MAC			0x7f0016
+	memcpy_fromio(&ltq_eth_data.mac.sa_data,
+		(void *)KSEG1ADDR(LTQ_FLASH_START + ARV75XX_BRN_MAC), 6);
+	ltq_register_etop(&ltq_eth_data);
+}
+
+static void
+bewan_register_ethernet(void)
+{
+#define BEWAN_BRN_MAC			0x3f0014
+	memcpy_fromio(&ltq_eth_data.mac.sa_data,
+		(void *)KSEG1ADDR(LTQ_FLASH_START + BEWAN_BRN_MAC), 6);
+	ltq_register_etop(&ltq_eth_data);
+}
+
+/*static u16 arv45xx_ath5k_eeprom_data[ATH5K_PLAT_EEP_MAX_WORDS];
+static struct ath5k_platform_data arv45xx_ath5k_platform_data;
+
+static int arv45xx_pci_plat_dev_init(struct pci_dev *dev)
+{
+	dev->dev.platform_data = &arv45xx_ath5k_platform_data;
+	return 0;
+}
+
+void __init
+arv45xx_register_ath5k(void)
+{
+#define ARV45XX_BRN_ATH		0x3f0478
+	int i;
+	unsigned char eeprom_mac[6];
+	static u16 eeprom_data[ATH5K_PLAT_EEP_MAX_WORDS];
+	u32 *p = (u32*)arv45xx_ath5k_eeprom_data;
+
+	memcpy_fromio(eeprom_mac,
+		(void *)KSEG1ADDR(LTQ_FLASH_START + ARV45XX_BRN_MAC), 6);
+	eeprom_mac[5]++;
+	memcpy_fromio(arv45xx_ath5k_eeprom_data,
+		(void *)KSEG1ADDR(LTQ_FLASH_START + ARV45XX_BRN_ATH), ATH5K_PLAT_EEP_MAX_WORDS);
+	// swap eeprom bytes
+	for (i = 0; i < ATH5K_PLAT_EEP_MAX_WORDS>>1; i++){
+		//arv4518_ath5k_eeprom_data[i] = ((eeprom_data[i]&0xff)<<8)|((eeprom_data[i]&0xff00)>>8);
+		p[i] = ((eeprom_data[(i<<1)+1]&0xff)<<24)|((eeprom_data[(i<<1)+1]&0xff00)<<8)|((eeprom_data[i<<1]&0xff)<<8)|((eeprom_data[i<<1]&0xff00)>>8);
+		if (i == 0xbf>>1){
+			// printk ("regdomain: 0x%x --> 0x%x\n", p[i], (p[i] & 0xffff0000)|0x67);
+			// regdomain is invalid?? how did original fw convert 
+			// value to 0x82d4 ??
+			// for now, force to 0x67
+			p[i] &= 0xffff0000;
+			p[i] |= 0x67;
+		}
+	}
+	arv45xx_ath5k_platform_data.eeprom_data = arv45xx_ath5k_eeprom_data;
+	arv45xx_ath5k_platform_data.macaddr = eeprom_mac;
+	//lqpci_plat_dev_init = arv45xx_pci_plat_dev_init;
+}*/
+
+static void __init
+arv3527p_init(void)
+{
+	ltq_register_gpio_stp();
+	//ltq_add_device_leds_gpio(arv3527p_leds_gpio, ARRAY_SIZE(arv3527p_leds_gpio));
+	ltq_register_nor(&arv45xx_flash_data);
+	arv45xx_register_ethernet();
+}
+
+MIPS_MACHINE(LANTIQ_MACH_ARV3527P,
+			"ARV3527P",
+			"ARV3527P - Arcor Easybox 401",
+			arv3527p_init);
+
+static void __init
+arv4510pw_init(void)
+{
+	ltq_register_gpio_stp();
+	ltq_add_device_leds_gpio(-1, ARRAY_SIZE(arv4510pw_leds_gpio), arv4510pw_leds_gpio);
+	ltq_register_nor(&arv4510_flash_data);
+	ltq_pci_data.irq[12] = (INT_NUM_IM2_IRL0 + 31);
+	ltq_pci_data.irq[15] = (INT_NUM_IM0_IRL0 + 26);
+	ltq_pci_data.gpio |= PCI_EXIN2 | PCI_REQ2;
+	ltq_register_pci(&ltq_pci_data);
+	bewan_register_ethernet();
+}
+
+MIPS_MACHINE(LANTIQ_MACH_ARV4510PW,
+			"ARV4510PW",
+			"ARV4510PW - Wippies Homebox",
+			arv4510pw_init);
+
+static void __init
+arv4518pw_init(void)
+{
+#define ARV4518PW_EBU			0
+#define ARV4518PW_USB			14
+#define ARV4518PW_SWITCH_RESET		13
+
+	ltq_register_gpio_ebu(ARV4518PW_EBU);
+	ltq_add_device_leds_gpio(-1, ARRAY_SIZE(arv4518pw_leds_gpio), arv4518pw_leds_gpio);
+	ltq_register_gpio_buttons(arv4518pw_gpio_buttons, ARRAY_SIZE(arv4518pw_gpio_buttons));
+	ltq_register_nor(&arv45xx_flash_data);
+	ltq_pci_data.gpio = PCI_GNT2 | PCI_REQ2;
+	ltq_register_pci(&ltq_pci_data);
+	ltq_register_madwifi_eep();
+	xway_register_dwc(ARV4518PW_USB);
+	arv45xx_register_ethernet();
+//	arv45xx_register_ath5k();
+
+	gpio_request(ARV4518PW_SWITCH_RESET, "switch");
+	gpio_direction_output(ARV4518PW_SWITCH_RESET, 1);
+	gpio_export(ARV4518PW_SWITCH_RESET, 0);
+}
+
+MIPS_MACHINE(LANTIQ_MACH_ARV4518PW,
+			"ARV4518PW",
+			"ARV4518PW - SMC7908A-ISP, Airties WAV-221",
+			arv4518pw_init);
+
+static void __init
+arv4520pw_init(void)
+{
+#define ARV4520PW_EBU			0x400
+#define ARV4520PW_USB			28
+#define ARV4520PW_SWITCH_RESET		82
+
+	ltq_register_gpio_ebu(ARV4520PW_EBU);
+	ltq_add_device_leds_gpio(-1, ARRAY_SIZE(arv4520pw_leds_gpio), arv4520pw_leds_gpio);
+	ltq_register_nor(&arv45xx_flash_data);
+	ltq_register_pci(&ltq_pci_data);
+	ltq_register_tapi();
+	arv45xx_register_ethernet();
+	xway_register_dwc(ARV4520PW_USB);
+
+	gpio_request(ARV4520PW_SWITCH_RESET, "switch");
+	gpio_set_value(ARV4520PW_SWITCH_RESET, 1);
+}
+
+MIPS_MACHINE(LANTIQ_MACH_ARV4520PW,
+			"ARV4520PW",
+			"ARV4520PW - Airties WAV-281, Arcor A800",
+			arv4520pw_init);
+
+static void __init
+arv452Cpw_init(void)
+{
+#define ARV452CPW_EBU			0x77f
+#define ARV452CPW_USB			28
+#define ARV452CPW_RELAY1		31
+#define ARV452CPW_RELAY2		79
+#define ARV452CPW_SWITCH_RESET		82
+
+	ltq_register_gpio_ebu(ARV452CPW_EBU);
+	ltq_add_device_leds_gpio(-1, ARRAY_SIZE(arv452cpw_leds_gpio), arv452cpw_leds_gpio);
+	ltq_register_nor(&arv45xx_flash_data);
+	ltq_register_pci(&ltq_pci_data);
+	ltq_register_madwifi_eep();
+	xway_register_dwc(ARV452CPW_USB);
+	arv45xx_register_ethernet();
+//	arv45xx_register_ath5k();
+
+	gpio_request(ARV452CPW_SWITCH_RESET, "switch");
+	gpio_set_value(ARV452CPW_SWITCH_RESET, 1);
+	gpio_export(ARV452CPW_SWITCH_RESET, 0);
+
+	gpio_request(ARV452CPW_RELAY1, "relay1");
+	gpio_direction_output(ARV452CPW_RELAY1, 1);
+	gpio_export(ARV452CPW_RELAY1, 0);
+
+	gpio_request(ARV452CPW_RELAY2, "relay2");
+	gpio_set_value(ARV452CPW_RELAY2, 1);
+	gpio_export(ARV452CPW_RELAY2, 0);
+}
+
+MIPS_MACHINE(LANTIQ_MACH_ARV452CPW,
+			"ARV452CPW",
+			"ARV452CPW - Arcor A801",
+			arv452Cpw_init);
+
+static void __init
+arv4525pw_init(void)
+{
+	ltq_add_device_leds_gpio(-1, ARRAY_SIZE(arv4525pw_leds_gpio), arv4525pw_leds_gpio);
+	ltq_register_nor(&arv45xx_flash_data);
+	ltq_pci_data.clock = PCI_CLOCK_INT;
+	ltq_register_pci(&ltq_pci_data);
+	ltq_register_madwifi_eep();
+	ltq_eth_data.mii_mode = PHY_INTERFACE_MODE_MII;
+	arv45xx_register_ethernet();
+}
+
+MIPS_MACHINE(LANTIQ_MACH_ARV4525PW,
+			"ARV4525PW",
+			"ARV4525PW - Speedport W502V",
+			arv4525pw_init);
+
+static void __init
+arv7518pw_init(void)
+{
+#define ARV7518PW_EBU			0x2
+#define ARV7518PW_USB			14
+
+	ltq_register_gpio_ebu(ARV7518PW_EBU);
+	ltq_add_device_leds_gpio(-1, ARRAY_SIZE(arv7518pw_leds_gpio), arv7518pw_leds_gpio);
+	ltq_register_gpio_buttons(arv7518pw_gpio_buttons, ARRAY_SIZE(arv7518pw_gpio_buttons));
+	ltq_register_nor(&arv75xx_flash_data);
+	ltq_register_pci(&ltq_pci_data);
+	ltq_register_tapi();
+	xway_register_dwc(ARV7518PW_USB);
+	arv75xx_register_ethernet();
+	//arv7518_register_ath9k(mac);
+}
+
+MIPS_MACHINE(LANTIQ_MACH_ARV7518PW,
+			"ARV7518PW",
+			"ARV7518PW - ASTORIA",
+			arv7518pw_init);
+
+static void __init
+arv752dpw22_init(void)
+{
+#define ARV752DPW22_EBU			0x2
+#define ARV752DPW22_USB			72
+#define ARV752DPW22_RELAY		73
+
+	ltq_register_gpio_ebu(ARV752DPW22_EBU);
+	ltq_add_device_leds_gpio(-1, ARRAY_SIZE(arv752dpw22_leds_gpio), arv752dpw22_leds_gpio);
+	ltq_register_gpio_buttons(arv752dpw22_gpio_buttons, ARRAY_SIZE(arv752dpw22_gpio_buttons));
+	ltq_register_nor(&arv75xx_flash_data);
+	ltq_pci_data.irq[15] = (INT_NUM_IM2_IRL0 + 31);
+	ltq_pci_data.gpio |= PCI_EXIN1 | PCI_REQ2;
+	ltq_register_pci(&ltq_pci_data);
+	xway_register_dwc(ARV752DPW22_USB);
+	arv75xx_register_ethernet();
+
+	gpio_request(ARV752DPW22_RELAY, "relay");
+	gpio_set_value(ARV752DPW22_RELAY, 1);
+	gpio_export(ARV752DPW22_RELAY, 0);
+}
+
+MIPS_MACHINE(LANTIQ_MACH_ARV752DPW22,
+			"ARV752DPW22",
+			"ARV752DPW22 - Arcor A803",
+			arv752dpw22_init);
--- a/arch/mips/lantiq/machtypes.h
+++ b/arch/mips/lantiq/machtypes.h
@@ -21,6 +21,17 @@
 	LANTIQ_MACH_EASY98000SF,	/* Falcon Eval Board, Serial Flash */
 	LANTIQ_MACH_EASY98020,		/* Falcon Reference Board */
 	LANTIQ_MACH_95C3AM1,		/* Board 95C3AM1 */
+
+	/* Arcadyan */
+	LANTIQ_MACH_ARV3527P,		/* Arcor easybox a401 */
+	LANTIQ_MACH_ARV4510PW,		/* Wippies Homebox */
+	LANTIQ_MACH_ARV4518PW,		/* Airties WAV-221, SMC-7908A-ISP */
+	LANTIQ_MACH_ARV4520PW,		/* Airties WAV-281, Arcor EasyboxA800 */
+	LANTIQ_MACH_ARV452CPW,		/* Arcor EasyboxA801 */
+	LANTIQ_MACH_ARV4525PW,		/* Speedport W502V */
+	LANTIQ_MACH_ARV752DPW,		/* Arcor easybox a802 */
+	LANTIQ_MACH_ARV752DPW22,	/* Arcor easybox a803 */
+	LANTIQ_MACH_ARV7518PW,		/* ASTORIA */
 };
 
 #endif
