From 436aee004fda70b654698aff99427abdebf6bdb9 Mon Sep 17 00:00:00 2001
From: Lars-Peter Clausen <lars@metafoo.de>
Date: Mon, 11 Jan 2010 04:29:37 +0100
Subject: [PATCH] /opt/Projects/openwrt/target/linux/xburst/patches-2.6.31/050-nand.patch

---
 drivers/mtd/nand/Kconfig     |    6 ++++++
 drivers/mtd/nand/Makefile    |    1 +
 drivers/mtd/nand/nand_base.c |   19 +++++++------------
 3 files changed, 14 insertions(+), 12 deletions(-)

--- a/drivers/mtd/nand/Kconfig
+++ b/drivers/mtd/nand/Kconfig
@@ -482,4 +482,10 @@ config MTD_NAND_W90P910
 	  This enables the driver for the NAND Flash on evaluation board based
 	  on w90p910.
 
+config MTD_NAND_JZ4740
+	tristate "Support NAND Flash device on Jz4740 board"
+	depends on SOC_JZ4740
+	help
+	Support NAND Flash device on Jz4740 board
+
 endif # MTD_NAND
--- a/drivers/mtd/nand/Makefile
+++ b/drivers/mtd/nand/Makefile
@@ -42,5 +42,6 @@ obj-$(CONFIG_MTD_NAND_SOCRATES)		+= socr
 obj-$(CONFIG_MTD_NAND_TXX9NDFMC)	+= txx9ndfmc.o
 obj-$(CONFIG_MTD_NAND_W90P910)		+= w90p910_nand.o
 obj-$(CONFIG_MTD_NAND_NOMADIK)		+= nomadik_nand.o
+obj-$(CONFIG_MTD_NAND_JZ4740)		+= jz4740_nand.o
 
 nand-objs := nand_base.o nand_bbt.o
