--- a/drivers/leds/Kconfig
+++ b/drivers/leds/Kconfig
@@ -236,6 +236,13 @@ config LEDS_BD2802
 	  This option enables support for BD2802GU RGB LED driver chips
 	  accessed via the I2C bus.
 
+config LEDS_WNDR3700_USB
+	tristate "NETGEAR WNDR3700 USB LED driver"
+	depends on LEDS_CLASS && AR71XX_MACH_WNDR3700
+	help
+	  This option enables support for the USB LED found on the
+	  NETGEAR WNDR3700 board.
+
 comment "LED Triggers"
 
 config LEDS_TRIGGERS
--- a/drivers/leds/Makefile
+++ b/drivers/leds/Makefile
@@ -29,6 +29,7 @@ obj-$(CONFIG_LEDS_DA903X)		+= leds-da903
 obj-$(CONFIG_LEDS_WM831X_STATUS)	+= leds-wm831x-status.o
 obj-$(CONFIG_LEDS_WM8350)		+= leds-wm8350.o
 obj-$(CONFIG_LEDS_PWM)			+= leds-pwm.o
+obj-${CONFIG_LEDS_WNDR3700_USB}		+= leds-wndr3700-usb.o
 
 # LED SPI Drivers
 obj-$(CONFIG_LEDS_DAC124S085)		+= leds-dac124s085.o
