--- a/drivers/usb/host/adm5120-dbg.c
+++ b/drivers/usb/host/adm5120-dbg.c
@@ -419,7 +419,7 @@ static struct dentry *admhc_debug_root;
 
 struct debug_buffer {
 	ssize_t (*fill_func)(struct debug_buffer *);    /* fill method */
-	struct device *dev;
+	struct admhcd *ahcd;
 	struct mutex mutex;     /* protect filling of buffer */
 	size_t count;           /* number of characters filled into buffer */
 	char *page;
@@ -494,15 +494,11 @@ show_list(struct admhcd *ahcd, char *buf
 
 static ssize_t fill_async_buffer(struct debug_buffer *buf)
 {
-	struct usb_bus		*bus;
-	struct usb_hcd		*hcd;
 	struct admhcd		*ahcd;
 	size_t			temp;
 	unsigned long		flags;
 
-	bus = dev_get_drvdata(buf->dev);
-	hcd = bus_to_hcd(bus);
-	ahcd = hcd_to_admhcd(hcd);
+	ahcd = buf->ahcd;
 
 	spin_lock_irqsave(&ahcd->lock, flags);
 	temp = show_list(ahcd, buf->page, PAGE_SIZE, ahcd->ed_head);
@@ -516,8 +512,6 @@ static ssize_t fill_async_buffer(struct 
 
 static ssize_t fill_periodic_buffer(struct debug_buffer *buf)
 {
-	struct usb_bus		*bus;
-	struct usb_hcd		*hcd;
 	struct admhcd		*ahcd;
 	struct ed		**seen, *ed;
 	unsigned long		flags;
@@ -529,9 +523,7 @@ static ssize_t fill_periodic_buffer(stru
 		return 0;
 	seen_count = 0;
 
-	bus = dev_get_drvdata(buf->dev);
-	hcd = bus_to_hcd(bus);
-	ahcd = hcd_to_admhcd(hcd);
+	ahcd = buf->ahcd;
 	next = buf->page;
 	size = PAGE_SIZE;
 
@@ -613,7 +605,6 @@ static ssize_t fill_periodic_buffer(stru
 
 static ssize_t fill_registers_buffer(struct debug_buffer *buf)
 {
-	struct usb_bus		*bus;
 	struct usb_hcd		*hcd;
 	struct admhcd		*ahcd;
 	struct admhcd_regs __iomem *regs;
@@ -622,9 +613,8 @@ static ssize_t fill_registers_buffer(str
 	char			*next;
 	u32			rdata;
 
-	bus = dev_get_drvdata(buf->dev);
-	hcd = bus_to_hcd(bus);
-	ahcd = hcd_to_admhcd(hcd);
+	ahcd = buf->ahcd;
+	hcd = admhcd_to_hcd(ahcd);
 	regs = ahcd->regs;
 	next = buf->page;
 	size = PAGE_SIZE;
@@ -689,7 +679,7 @@ done:
 }
 
 
-static struct debug_buffer *alloc_buffer(struct device *dev,
+static struct debug_buffer *alloc_buffer(struct admhcd *ahcd,
 				ssize_t (*fill_func)(struct debug_buffer *))
 {
 	struct debug_buffer *buf;
@@ -697,7 +687,7 @@ static struct debug_buffer *alloc_buffer
 	buf = kzalloc(sizeof(struct debug_buffer), GFP_KERNEL);
 
 	if (buf) {
-		buf->dev = dev;
+		buf->ahcd = ahcd;
 		buf->fill_func = fill_func;
 		mutex_init(&buf->mutex);
 	}
@@ -790,26 +780,25 @@ static int debug_registers_open(struct i
 static inline void create_debug_files(struct admhcd *ahcd)
 {
 	struct usb_bus *bus = &admhcd_to_hcd(ahcd)->self;
-	struct device *dev = bus->dev;
 
 	ahcd->debug_dir = debugfs_create_dir(bus->bus_name, admhc_debug_root);
 	if (!ahcd->debug_dir)
 		goto dir_error;
 
 	ahcd->debug_async = debugfs_create_file("async", S_IRUGO,
-						ahcd->debug_dir, dev,
+						ahcd->debug_dir, ahcd,
 						&debug_async_fops);
 	if (!ahcd->debug_async)
 		goto async_error;
 
 	ahcd->debug_periodic = debugfs_create_file("periodic", S_IRUGO,
-						ahcd->debug_dir, dev,
+						ahcd->debug_dir, ahcd,
 						&debug_periodic_fops);
 	if (!ahcd->debug_periodic)
 		goto periodic_error;
 
 	ahcd->debug_registers = debugfs_create_file("registers", S_IRUGO,
-						ahcd->debug_dir, dev,
+						ahcd->debug_dir, ahcd,
 						&debug_registers_fops);
 	if (!ahcd->debug_registers)
 		goto registers_error;
