--- a/drivers/leds/Kconfig
+++ b/drivers/leds/Kconfig
@@ -315,4 +315,12 @@ config LEDS_TRIGGER_NETDEV
 	  This allows LEDs to be controlled by network device activity.
 	  If unsure, say Y.
 
+config LEDS_TRIGGER_ADM5120_SWITCH
+	tristate "LED ADM5120 Switch Port Status Trigger"
+	depends on LEDS_TRIGGERS && ADM5120
+	help
+	  This allows LEDs to be controlled by the port states of
+	  the ADM5120 built-in Ethernet Switch
+	  If unsure, say N.
+
 endif # NEW_LEDS
--- a/drivers/leds/Makefile
+++ b/drivers/leds/Makefile
@@ -42,3 +42,4 @@ obj-$(CONFIG_LEDS_TRIGGER_GPIO)		+= ledt
 obj-$(CONFIG_LEDS_TRIGGER_DEFAULT_ON)	+= ledtrig-default-on.o
 obj-$(CONFIG_LEDS_TRIGGER_MORSE)	+= ledtrig-morse.o
 obj-$(CONFIG_LEDS_TRIGGER_NETDEV)      += ledtrig-netdev.o
+obj-$(CONFIG_LEDS_TRIGGER_ADM5120_SWITCH) += ledtrig-adm5120-switch.o
