From 72a9b536ef81f06bb8042abee0410458f5df93d2 Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Fri, 6 May 2011 00:10:02 +0200
Subject: [PATCH 12/13] MIPS: Lantiq: Add etop board support

Register the etop platform device inside the machtype specific init code.

Signed-off-by: John Crispin <blogic@openwrt.org>
Signed-off-by: Ralph Hempel <ralph.hempel@lantiq.com>
Signed-off-by: David Daney <ddaney@caviumnetworks.com>
Cc: linux-mips@linux-mips.org
Patchwork: https://patchwork.linux-mips.org/patch/2356/
Patchwork: https://patchwork.linux-mips.org/patch/2370/
Signed-off-by: Ralf Baechle <ralf@linux-mips.org>
---
 arch/mips/lantiq/xway/mach-easy50712.c |    6 ++++++
 1 files changed, 6 insertions(+), 0 deletions(-)

diff --git a/arch/mips/lantiq/xway/mach-easy50712.c b/arch/mips/lantiq/xway/mach-easy50712.c
index e5e7e09..ea5027b 100644
--- a/arch/mips/lantiq/xway/mach-easy50712.c
+++ b/arch/mips/lantiq/xway/mach-easy50712.c
@@ -12,6 +12,7 @@
 #include <linux/mtd/partitions.h>
 #include <linux/mtd/physmap.h>
 #include <linux/input.h>
+#include <linux/phy.h>
 
 #include <lantiq_soc.h>
 #include <irq.h>
@@ -55,11 +56,16 @@ static struct ltq_pci_data ltq_pci_data = {
 	},
 };
 
+static struct ltq_eth_data ltq_eth_data = {
+	.mii_mode = PHY_INTERFACE_MODE_MII,
+};
+
 static void __init easy50712_init(void)
 {
 	ltq_register_gpio_stp();
 	ltq_register_nor(&easy50712_flash_data);
 	ltq_register_pci(&ltq_pci_data);
+	ltq_register_etop(&ltq_eth_data);
 }
 
 MIPS_MACHINE(LTQ_MACH_EASY50712,
-- 
1.7.2.3

