--- a/arch/mips/bcm63xx/boards/Kconfig
+++ b/arch/mips/bcm63xx/boards/Kconfig
@@ -8,4 +8,10 @@ config BOARD_BCM963XX
 	select SSB
        help
 
+config BOARD_LIVEBOX
+	bool "Inventel Livebox(es) boards"
+	select SSB
+	help
+	 Inventel Livebox boards using the RedBoot bootloader.
+
 endchoice
--- a/arch/mips/bcm63xx/boards/Makefile
+++ b/arch/mips/bcm63xx/boards/Makefile
@@ -1,3 +1,4 @@
 obj-$(CONFIG_BOARD_BCM963XX)		+= board_bcm963xx.o
+obj-$(CONFIG_BOARD_LIVEBOX)		+= board_livebox.o
 
 EXTRA_CFLAGS += -Werror
--- /dev/null
+++ b/arch/mips/bcm63xx/boards/board_livebox.c
@@ -0,0 +1,223 @@
+/*
+ * This file is subject to the terms and conditions of the GNU General Public
+ * License.  See the file "COPYING" in the main directory of this archive
+ * for more details.
+ *
+ * Copyright (C) 2008 Florian Fainelli <florian@openwrt.org>
+ */
+
+#include <linux/init.h>
+#include <linux/kernel.h>
+#include <linux/string.h>
+#include <linux/platform_device.h>
+#include <linux/mtd/mtd.h>
+#include <linux/mtd/partitions.h>
+#include <linux/mtd/physmap.h>
+#include <linux/input.h>
+#include <linux/gpio_buttons.h>
+#include <asm/addrspace.h>
+#include <bcm63xx_board.h>
+#include <bcm63xx_cpu.h>
+#include <bcm63xx_regs.h>
+#include <bcm63xx_io.h>
+#include <bcm63xx_dev_pci.h>
+#include <bcm63xx_dev_enet.h>
+#include <bcm63xx_dev_pcmcia.h>
+#include <bcm63xx_dev_usb_ohci.h>
+#include <bcm63xx_dev_usb_ehci.h>
+#include <board_bcm963xx.h>
+
+#define PFX	"board_livebox: "
+
+static unsigned int mac_addr_used = 0;
+static struct board_info board;
+
+/*
+ * known 6348 boards
+ */
+#ifdef CONFIG_BCM63XX_CPU_6348
+static struct board_info __initdata board_livebox = {
+	.name				= "Livebox",
+	.expected_cpu_id		= 0x6348,
+
+	.has_enet0			= 1,
+	.has_enet1			= 1,
+	.has_pci			= 1,
+
+	.enet0 = {
+		.has_phy		= 1,
+		.use_internal_phy	= 1,
+	},
+
+	.enet1 = {
+		.force_speed_100	= 1,
+		.force_duplex_full	= 1,
+	},
+
+	.has_ohci0			= 1,
+	.has_pccard			= 1,
+	.has_ehci0			= 1,
+};
+#endif
+
+/*
+ * all boards
+ */
+static const struct board_info __initdata *bcm963xx_boards[] = {
+#ifdef CONFIG_BCM63XX_CPU_6348
+	&board_livebox
+#endif
+};
+
+/*
+ * early init callback
+ */
+void __init board_prom_init(void)
+{
+	u32 val;
+
+	/* read base address of boot chip select (0) */
+	val = bcm_mpi_readl(MPI_CSBASE_REG(0));
+	val &= MPI_CSBASE_BASE_MASK;
+
+	/* assume board is a Livebox */
+	memcpy(&board, bcm963xx_boards[0], sizeof(board));
+
+	/* setup pin multiplexing depending on board enabled device,
+	 * this has to be done this early since PCI init is done
+	 * inside arch_initcall */
+	val = 0;
+
+	if (board.has_pci) {
+		bcm63xx_pci_enabled = 1;
+		if (BCMCPU_IS_6348())
+			val |= GPIO_MODE_6348_G2_PCI;
+	}
+
+	if (board.has_pccard) {
+		if (BCMCPU_IS_6348())
+			val |= GPIO_MODE_6348_G1_MII_PCCARD;
+	}
+
+	if (board.has_enet0 && !board.enet0.use_internal_phy) {
+		if (BCMCPU_IS_6348())
+			val |= GPIO_MODE_6348_G3_EXT_MII |
+				GPIO_MODE_6348_G0_EXT_MII;
+	}
+
+	if (board.has_enet1 && !board.enet1.use_internal_phy) {
+		if (BCMCPU_IS_6348())
+			val |= GPIO_MODE_6348_G3_EXT_MII |
+				GPIO_MODE_6348_G0_EXT_MII;
+	}
+
+	bcm_gpio_writel(val, GPIO_MODE_REG);
+}
+
+/*
+ * second stage init callback, good time to panic if we couldn't
+ * identify on which board we're running since early printk is working
+ */
+void __init board_setup(void)
+{
+	if (!board.name[0])
+		panic("unable to detect bcm963xx board");
+	printk(KERN_INFO PFX "board name: %s\n", board.name);
+
+	/* make sure we're running on expected cpu */
+	if (bcm63xx_get_cpu_id() != board.expected_cpu_id)
+		panic("unexpected CPU for bcm963xx board");
+}
+
+/*
+ * return board name for /proc/cpuinfo
+ */
+const char *board_get_name(void)
+{
+	return board.name;
+}
+
+/*
+ * register & return a new board mac address
+ */
+
+static int board_get_mac_address(u8 *mac)
+{
+	u8 default_mac[ETH_ALEN] = {0x00, 0x07, 0x3A, 0x00, 0x00, 0x00};
+	u8 *p;
+	int count;
+
+	memcpy(mac, default_mac, ETH_ALEN);
+
+	p = mac + ETH_ALEN - 1;
+	count = mac_addr_used;
+
+	while (count--) {
+		do {
+			(*p)++;
+			if (*p != 0)
+				break;
+			p--;
+		} while (p != mac);
+	}
+
+	if (p == mac) {
+		printk(KERN_ERR PFX "unable to fetch mac address\n");
+		return -ENODEV;
+	}
+        mac_addr_used++;
+
+	return 0;
+}
+
+static struct resource mtd_resources[] = {
+	{
+		.start          = 0,    /* filled at runtime */
+		.end            = 0,    /* filled at runtime */
+		.flags          = IORESOURCE_MEM,
+	}
+};
+
+static struct platform_device mtd_dev = {
+	.name                   = "bcm963xx-flash",
+	.resource               = mtd_resources,
+	.num_resources          = ARRAY_SIZE(mtd_resources),
+};
+
+
+/*
+ * third stage init callback, register all board devices.
+ */
+int __init board_register_devices(void)
+{
+	u32 val;
+
+	if (board.has_pccard)
+		bcm63xx_pcmcia_register();
+
+	if (board.has_enet0 &&
+	    !board_get_mac_address(board.enet0.mac_addr))
+		bcm63xx_enet_register(0, &board.enet0);
+
+	if (board.has_enet1 &&
+	    !board_get_mac_address(board.enet1.mac_addr))
+		bcm63xx_enet_register(1, &board.enet1);
+
+	if (board.has_ohci0)
+		bcm63xx_ohci_register();
+
+	if (board.has_ehci0)
+		bcm63xx_ehci_register();
+
+
+	/* read base address of boot chip select (0) */
+	val = bcm_mpi_readl(MPI_CSBASE_REG(0));
+	val &= MPI_CSBASE_BASE_MASK;
+	mtd_resources[0].start = val;
+	mtd_resources[0].end = 0x1FFFFFFF;
+
+	platform_device_register(&mtd_dev);
+
+	return 0;
+}
+
