From e734ace5baa04e0e8af1d4483475fbd6bd2b32a1 Mon Sep 17 00:00:00 2001
From: Axel Gembe <ago@bastart.eu.org>
Date: Mon, 12 May 2008 18:54:09 +0200
Subject: [PATCH] bcm963xx: flashmap support


Signed-off-by: Axel Gembe <ago@bastart.eu.org>
---
 drivers/mtd/maps/Kconfig  |    7 +++++++
 drivers/mtd/maps/Makefile |    1 +
 drivers/mtd/redboot.c     |   13 ++++++++++---
 3 files changed, 18 insertions(+), 3 deletions(-)

Index: linux-2.6.32.10/drivers/mtd/maps/Kconfig
===================================================================
--- linux-2.6.32.10.orig/drivers/mtd/maps/Kconfig	2010-03-29 06:35:59.987293878 -0400
+++ linux-2.6.32.10/drivers/mtd/maps/Kconfig	2010-03-29 06:37:14.968545954 -0400
@@ -259,6 +259,13 @@
 	help
 	  Flash memory access on AMD Alchemy Pb/Db/RDK Reference Boards
 
+config MTD_BCM963XX
+        tristate "BCM963xx Flash device"
+        depends on MIPS && BCM63XX
+        help
+	  Flash memory access on BCM963xx boards. Currently only works with
+	  RedBoot and CFE.
+
 config MTD_DILNETPC
 	tristate "CFI Flash device mapped on DIL/Net PC"
 	depends on X86 && MTD_CONCAT && MTD_PARTITIONS && MTD_CFI_INTELEXT && BROKEN
Index: linux-2.6.32.10/drivers/mtd/redboot.c
===================================================================
--- linux-2.6.32.10.orig/drivers/mtd/redboot.c	2010-03-29 06:36:00.017292877 -0400
+++ linux-2.6.32.10/drivers/mtd/redboot.c	2010-03-29 06:37:14.968545954 -0400
@@ -39,7 +39,7 @@
 	return 1;
 }
 
-static int parse_redboot_partitions(struct mtd_info *master,
+int parse_redboot_partitions(struct mtd_info *master,
                              struct mtd_partition **pparts,
                              unsigned long fis_origin)
 {
@@ -162,6 +162,14 @@
 		goto out;
 	}
 
+	if (!fis_origin) {
+		for (i = 0; i < numslots; i++) {
+			if (!strncmp(buf[i].name, "RedBoot", 8)) {
+				fis_origin = (buf[i].flash_base & (master->size << 1) - 1);
+			}
+		}
+	}
+
 	for (i = 0; i < numslots; i++) {
 		struct fis_list *new_fl, **prev;
 
@@ -184,9 +192,8 @@
 		new_fl->img = &buf[i];
                 if (fis_origin) {
                         buf[i].flash_base -= fis_origin;
-                } else {
-                        buf[i].flash_base &= master->size-1;
                 }
+		buf[i].flash_base &= (master->size << 1) - 1;
 
 		/* I'm sure the JFFS2 code has done me permanent damage.
 		 * I now think the following is _normal_
Index: linux-2.6.32.10/drivers/mtd/maps/Makefile
===================================================================
--- linux-2.6.32.10.orig/drivers/mtd/maps/Makefile	2010-03-29 06:35:59.947294290 -0400
+++ linux-2.6.32.10/drivers/mtd/maps/Makefile	2010-03-29 06:37:14.968545954 -0400
@@ -61,3 +61,4 @@
 obj-$(CONFIG_MTD_RBTX4939)	+= rbtx4939-flash.o
 obj-$(CONFIG_MTD_VMU)		+= vmu-flash.o
 obj-$(CONFIG_MTD_GPIO_ADDR)	+= gpio-addr-flash.o
+obj-$(CONFIG_MTD_BCM963XX)	+= bcm963xx-flash.o
Index: linux-2.6.32.10/drivers/mtd/maps/bcm963xx-flash.c
===================================================================
--- /dev/null	1970-01-01 00:00:00.000000000 +0000
+++ linux-2.6.32.10/drivers/mtd/maps/bcm963xx-flash.c	2010-03-29 13:33:58.797288897 -0400
@@ -0,0 +1,266 @@
+/*
+ * Copyright (C) 2006-2008  Florian Fainelli <florian@openwrt.org>
+ * 			    Mike Albon <malbon@openwrt.org>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301  USA
+ */
+
+#include <linux/init.h>
+#include <linux/kernel.h>
+#include <linux/mtd/map.h>
+#include <linux/mtd/mtd.h>
+#include <linux/mtd/partitions.h>
+#include <linux/vmalloc.h>
+#include <linux/platform_device.h>
+
+#include <bcm_tag.h>
+#include <asm/io.h>
+
+#define BUSWIDTH 2                     /* Buswidth */
+#define EXTENDED_SIZE 0xBFC00000       /* Extended flash address */
+
+#define PFX KBUILD_MODNAME ": "
+
+extern int parse_redboot_partitions(struct mtd_info *master, struct mtd_partition **pparts, unsigned long fis_origin);
+static struct mtd_partition *parsed_parts;
+
+static struct mtd_info *bcm963xx_mtd_info;
+
+static struct map_info bcm963xx_map = {
+       .name		= "bcm963xx",
+       .bankwidth	= BUSWIDTH,
+};
+
+
+static int parse_cfe_partitions( struct mtd_info *master, struct mtd_partition **pparts)
+{
+	int nrparts = 3, curpart = 0; /* CFE,NVRAM and global LINUX are always present. */
+	struct bcm_tag *buf;
+	struct mtd_partition *parts;
+	int ret;
+	size_t retlen;
+	unsigned int rootfsaddr, kerneladdr, spareaddr;
+	unsigned int rootfslen, kernellen, sparelen, totallen;
+	int namelen = 0;
+	int i;
+	char *boardid;
+        char *tagversion;
+
+	/* Allocate memory for buffer */
+	buf = vmalloc(sizeof(struct bcm_tag));
+	if (!buf)
+		return -ENOMEM;
+
+	/* Get the tag */
+	ret = master->read(master,master->erasesize,sizeof(struct bcm_tag), &retlen, (void *)buf);
+	if (retlen != sizeof(struct bcm_tag)){
+		vfree(buf);
+		return -EIO;
+	}
+
+	sscanf(buf->kernelAddress, "%u", &kerneladdr);
+	sscanf(buf->kernelLength, "%u", &kernellen);
+	sscanf(buf->totalLength, "%u", &totallen);
+	tagversion = &(buf->tagVersion[0]);
+	boardid = &(buf->boardid[0]);
+
+	printk(KERN_INFO PFX "CFE boot tag found with version %s and board type %s\n",tagversion, boardid);
+
+	kerneladdr = kerneladdr - EXTENDED_SIZE;
+	rootfsaddr = kerneladdr + kernellen;
+	spareaddr = roundup(totallen, master->erasesize) + master->erasesize;
+	sparelen = master->size - spareaddr - master->erasesize;
+	rootfslen = spareaddr - rootfsaddr;
+
+	/* Determine number of partitions */
+	namelen = 8;
+	if (rootfslen > 0){
+		nrparts++;
+		namelen =+ 6;
+	};
+	if (kernellen > 0) {
+		nrparts++;
+		namelen =+ 6;
+	};
+
+	/* Ask kernel for more memory */
+	parts = kzalloc(sizeof(*parts) * nrparts + 10 * nrparts, GFP_KERNEL);
+	if (!parts) {
+		vfree(buf);
+		return -ENOMEM;
+	};
+
+	/* Start building partition list */
+	parts[curpart].name = "CFE";
+	parts[curpart].offset = 0;
+	parts[curpart].size = master->erasesize;
+	curpart++;
+
+	if (kernellen > 0) {
+		parts[curpart].name = "kernel";
+		parts[curpart].offset = kerneladdr;
+		parts[curpart].size = kernellen;
+		curpart++;
+	};
+
+	if (rootfslen > 0) {
+		parts[curpart].name = "rootfs";
+		parts[curpart].offset = rootfsaddr;
+		parts[curpart].size = rootfslen;
+		if (sparelen > 0)
+			parts[curpart].size += sparelen;
+		curpart++;
+	};
+
+	parts[curpart].name = "nvram";
+	parts[curpart].offset = master->size - master->erasesize;
+	parts[curpart].size = master->erasesize;
+
+	/* Global partition "linux" to make easy firmware upgrade */
+	curpart++;
+	parts[curpart].name = "linux";
+	parts[curpart].offset = parts[0].size;
+	parts[curpart].size = master->size - parts[0].size - parts[3].size;
+
+	for (i = 0; i < nrparts; i++)
+		printk(KERN_INFO PFX "Partition %d is %s offset %lx and length %lx\n", i, parts[i].name, (long unsigned int)(parts[i].offset), (long unsigned int)(parts[i].size));
+
+ 	printk(KERN_INFO PFX "Spare partition is %x offset and length %x\n", spareaddr, sparelen);
+	*pparts = parts;
+	vfree(buf);
+
+	return nrparts;
+};
+
+static int bcm963xx_detect_cfe(struct mtd_info *master)
+{
+	int idoffset = 0x4e0;
+	static char idstring[8] = "CFE1CFE1";
+	char buf[9];
+	int ret;
+	size_t retlen;
+
+	ret = master->read(master, idoffset, 8, &retlen, (void *)buf);
+	buf[retlen] = 0;
+	printk(KERN_INFO PFX "Read Signature value of %s\n", buf);
+
+	return strncmp(idstring, buf, 8);
+}
+
+static int bcm963xx_probe(struct platform_device *pdev)
+{
+	int err = 0;
+	int parsed_nr_parts = 0;
+	char *part_type;
+	struct resource *r;
+
+	r = platform_get_resource(pdev, IORESOURCE_MEM, 0);
+	bcm963xx_map.phys = r->start;
+	bcm963xx_map.size = (r->end - r->start) + 1;
+	bcm963xx_map.virt = ioremap(r->start, r->end - r->start + 1);
+
+	if (!bcm963xx_map.virt) {
+		printk(KERN_ERR PFX "Failed to ioremap\n");
+		return -EIO;
+	}
+	printk(KERN_INFO PFX "0x%08lx at 0x%08x\n", bcm963xx_map.size, bcm963xx_map.phys);
+
+	simple_map_init(&bcm963xx_map);
+
+	bcm963xx_mtd_info = do_map_probe("cfi_probe", &bcm963xx_map);
+	if (!bcm963xx_mtd_info) {
+		printk(KERN_ERR PFX "Failed to probe using CFI\n");
+		err = -EIO;
+		goto err_probe;
+	}
+
+	bcm963xx_mtd_info->owner = THIS_MODULE;
+
+	/* This is mutually exclusive */
+	if (bcm963xx_detect_cfe(bcm963xx_mtd_info) == 0) {
+		printk(KERN_INFO PFX "CFE bootloader detected\n");
+		if (parsed_nr_parts == 0) {
+			int ret = parse_cfe_partitions(bcm963xx_mtd_info, &parsed_parts);
+			if (ret > 0) {
+				part_type = "CFE";
+				parsed_nr_parts = ret;
+			}
+		}
+	} else {
+		printk(KERN_INFO PFX "assuming RedBoot bootloader\n");
+		if (bcm963xx_mtd_info->size > 0x00400000) {
+			printk(KERN_INFO PFX "Support for extended flash memory size : 0x%lx ; ONLY 64MBIT SUPPORT\n", bcm963xx_mtd_info->size);
+			bcm963xx_map.virt = (u32)(EXTENDED_SIZE);
+		}
+
+#ifdef CONFIG_MTD_REDBOOT_PARTS
+		if (parsed_nr_parts == 0) {
+			int ret = parse_redboot_partitions(bcm963xx_mtd_info, &parsed_parts, 0);
+			if (ret > 0) {
+				part_type = "RedBoot";
+				parsed_nr_parts = ret;
+			}
+		}
+#endif
+	}
+
+	return add_mtd_partitions(bcm963xx_mtd_info, parsed_parts, parsed_nr_parts);
+
+err_probe:
+	iounmap(bcm963xx_map.virt);
+	return err;
+}
+
+static int bcm963xx_remove(struct platform_device *pdev)
+{
+	if (bcm963xx_mtd_info) {
+		del_mtd_partitions(bcm963xx_mtd_info);
+		map_destroy(bcm963xx_mtd_info);
+	}
+
+	if (bcm963xx_map.virt) {
+		iounmap(bcm963xx_map.virt);
+		bcm963xx_map.virt = 0;
+	}
+
+	return 0;
+}
+
+static struct platform_driver bcm63xx_mtd_dev = {
+	.probe	= bcm963xx_probe,
+	.remove = bcm963xx_remove,
+	.driver = {
+		.name	= "bcm963xx-flash",
+		.owner	= THIS_MODULE,
+	},
+};
+
+static int __init bcm963xx_mtd_init(void)
+{
+	return platform_driver_register(&bcm63xx_mtd_dev);
+}
+
+static void __exit bcm963xx_mtd_exit(void)
+{
+	platform_driver_unregister(&bcm63xx_mtd_dev);
+}
+
+module_init(bcm963xx_mtd_init);
+module_exit(bcm963xx_mtd_exit);
+
+MODULE_LICENSE("GPL");
+MODULE_DESCRIPTION("Broadcom BCM63xx MTD partition parser/mapping for CFE and RedBoot");
+MODULE_AUTHOR("Florian Fainelli <florian@openwrt.org>");
+MODULE_AUTHOR("Mike Albon <malbon@openwrt.org>");
Index: linux-2.6.32.10/arch/mips/bcm63xx/boards/board_bcm963xx.c
===================================================================
--- linux-2.6.32.10.orig/arch/mips/bcm63xx/boards/board_bcm963xx.c	2010-03-29 06:35:59.927292275 -0400
+++ linux-2.6.32.10/arch/mips/bcm63xx/boards/board_bcm963xx.c	2010-03-29 06:37:35.178541753 -0400
@@ -722,20 +722,6 @@
 	return 0;
 }
 
-static struct mtd_partition mtd_partitions[] = {
-	{
-		.name		= "cfe",
-		.offset		= 0x0,
-		.size		= 0x40000,
-	}
-};
-
-static struct physmap_flash_data flash_data = {
-	.width			= 2,
-	.nr_parts		= ARRAY_SIZE(mtd_partitions),
-	.parts			= mtd_partitions,
-};
-
 static struct resource mtd_resources[] = {
 	{
 		.start		= 0,	/* filled at runtime */
@@ -745,12 +731,9 @@
 };
 
 static struct platform_device mtd_dev = {
-	.name			= "physmap-flash",
+	.name			= "bcm963xx-flash",
 	.resource		= mtd_resources,
 	.num_resources		= ARRAY_SIZE(mtd_resources),
-	.dev			= {
-		.platform_data	= &flash_data,
-	},
 };
 
 /*
