From 806ead1e454a8a5876b777b22ca67187c4749f32 Mon Sep 17 00:00:00 2001
From: Lars-Peter Clausen <lars@metafoo.de>
Date: Mon, 11 Jan 2010 04:30:42 +0100
Subject: [PATCH] /opt/Projects/openwrt/target/linux/xburst/patches-2.6.31/800-n526-lpc.patch

---
 drivers/i2c/chips/Kconfig  |    9 +++++++++
 drivers/i2c/chips/Makefile |    1 +
 2 files changed, 10 insertions(+), 0 deletions(-)

--- a/drivers/i2c/chips/Kconfig
+++ b/drivers/i2c/chips/Kconfig
@@ -26,4 +26,21 @@ config SENSORS_TSL2550
 	  This driver can also be built as a module.  If so, the module
 	  will be called tsl2550.
 
+config N516_LPC
+	tristate "N516 keys & power controller"
+	depends on I2C
+	depends on INPUT
+	depends on POWER_SUPPLY
+	help
+	  N516 keyboard & power controller driver
+
+config N526_LPC
+	tristate "N526 LPC934 coprocessor"
+	depends on JZ4740_N526
+	help
+	  If you say yes here you get support for the N526s NXP LPC934 coprocessor.
+	  It is used as a keyboard controllor and for power management.
+
+	  If you have a N526 you probably want to say Y here.
+
 endmenu
--- a/drivers/i2c/chips/Makefile
+++ b/drivers/i2c/chips/Makefile
@@ -12,6 +12,8 @@
 
 obj-$(CONFIG_DS1682)		+= ds1682.o
 obj-$(CONFIG_SENSORS_TSL2550)	+= tsl2550.o
+obj-$(CONFIG_N516_LPC)		+= n516-lpc.o
+obj-$(CONFIG_N526_LPC)		+= n526-lpc.o
 
 ifeq ($(CONFIG_I2C_DEBUG_CHIP),y)
 EXTRA_CFLAGS += -DDEBUG
