bcm63xx_gpio_init is already called from prom_init to allow board to
use them early, so we can remove the unneeded arch_initcall.

Signed-off-by: Maxime Bizon <mbizon@freebox.fr>
---
 arch/mips/bcm63xx/gpio.c |    2 --
 1 files changed, 0 insertions(+), 2 deletions(-)

--- a/arch/mips/bcm63xx/gpio.c
+++ b/arch/mips/bcm63xx/gpio.c
@@ -130,5 +130,3 @@ int __init bcm63xx_gpio_init(void)
 
 	return gpiochip_add(&bcm63xx_gpio_chip);
 }
-
-arch_initcall(bcm63xx_gpio_init);
