Fix the usage of get_c0_compare_int: override cp0_compare_irq if the returned
value is in the MIPS CPU IRQ range to ensure that c0_compare_int_usable()
still works.

Signed-off-by: Felix Fietkau <nbd@openwrt.org>

--- a/arch/mips/kernel/cevt-r4k.c
+++ b/arch/mips/kernel/cevt-r4k.c
@@ -167,20 +167,23 @@ int __cpuinit r4k_clockevent_init(void)
 	struct clock_event_device *cd;
 	unsigned int irq;
 
-	if (!cpu_has_counter || !mips_hpt_frequency)
-		return -ENXIO;
-
-	if (!c0_compare_int_usable())
-		return -ENXIO;
-
 	/*
 	 * With vectored interrupts things are getting platform specific.
 	 * get_c0_compare_int is a hook to allow a platform to return the
 	 * interrupt number of it's liking.
 	 */
 	irq = MIPS_CPU_IRQ_BASE + cp0_compare_irq;
-	if (get_c0_compare_int)
+	if (get_c0_compare_int) {
 		irq = get_c0_compare_int();
+		if ((irq >= MIPS_CPU_IRQ_BASE) && (irq < MIPS_CPU_IRQ_BASE + 8))
+			cp0_compare_irq = irq - MIPS_CPU_IRQ_BASE;
+	}
+
+	if (!cpu_has_counter || !mips_hpt_frequency)
+		return -ENXIO;
+
+	if (!c0_compare_int_usable())
+		return -ENXIO;
 
 	cd = &per_cpu(mips_clockevent_device, cpu);
 
