--- a/drivers/mtd/maps/Kconfig
+++ b/drivers/mtd/maps/Kconfig
@@ -327,6 +327,12 @@ config MTD_CFI_FLAGADM
 	  Mapping for the Flaga digital module. If you don't have one, ignore
 	  this setting.
 
+config MTD_BCM47XX
+	tristate "BCM47xx flash device"
+	depends on MIPS && MTD_CFI && BCM47XX
+	help
+	  Support for the flash chips on the BCM947xx board.
+
 config MTD_REDWOOD
 	tristate "CFI Flash devices mapped on IBM Redwood"
 	depends on MTD_CFI && ( REDWOOD_4 || REDWOOD_5 || REDWOOD_6 )
--- a/drivers/mtd/maps/Makefile
+++ b/drivers/mtd/maps/Makefile
@@ -28,6 +28,7 @@ obj-$(CONFIG_MTD_PMC_MSP_EVM)   += pmcms
 obj-$(CONFIG_MTD_PCMCIA)	+= pcmciamtd.o
 obj-$(CONFIG_MTD_RPXLITE)	+= rpxlite.o
 obj-$(CONFIG_MTD_TQM8XXL)	+= tqm8xxl.o
+obj-$(CONFIG_MTD_BCM47XX)	+= bcm47xx-flash.o
 obj-$(CONFIG_MTD_SA1100)	+= sa1100-flash.o
 obj-$(CONFIG_MTD_IPAQ)		+= ipaq-flash.o
 obj-$(CONFIG_MTD_SBC_GXX)	+= sbc_gxx.o
