--- a/arch/mips/bcm63xx/boards/board_bcm963xx.c
+++ b/arch/mips/bcm63xx/boards/board_bcm963xx.c
@@ -336,24 +336,39 @@ static struct board_info __initdata boar
 			.active_low	= 1,
 		},
 		{
-			.name		= "ppp",
-			.gpio		= 3,
+			.name		= "power",
+			.gpio		= 0,
 			.active_low	= 1,
+			.default_trigger = "default-on",
 		},
 		{
-			.name		= "ppp-fail",
+			.name		= "stop",
+			.gpio		= 1,
+			.active_low	= 1,
+		},
+		{
+			.name		= "line1",
 			.gpio		= 4,
 			.active_low	= 1,
 		},
 		{
-			.name		= "power",
-			.gpio		= 0,
+			.name		= "line2",
+			.gpio		= 5,
 			.active_low	= 1,
-			.default_trigger = "default-on",
 		},
 		{
-			.name		= "stop",
-			.gpio		= 1,
+			.name		= "line3",
+			.gpio		= 6,
+			.active_low	= 1,
+		},
+		{
+			.name		= "tel",
+			.gpio		= 7,
+			.active_low	= 1,
+		},
+		{
+			.name		= "eth",
+			.gpio		= 35,
 			.active_low	= 1,
 		},
 	},
@@ -855,6 +870,7 @@ static struct platform_device bcm63xx_gp
 int __init board_register_devices(void)
 {
 	u32 val;
+	int led_count = 0;
 
 	if (board.has_pccard)
 		bcm63xx_pcmcia_register();
@@ -901,7 +917,11 @@ int __init board_register_devices(void)
 
 	platform_device_register_simple("GPIODEV", 0, &gpiodev_resource, 1);
 
-	bcm63xx_led_data.num_leds = ARRAY_SIZE(board.leds);
+	/* count number of LEDs defined by this device */
+	while (led_count < ARRAY_SIZE(board.leds) && board.leds[led_count].name)
+		led_count++;
+
+	bcm63xx_led_data.num_leds = led_count;
 	bcm63xx_led_data.leds = board.leds;
 
 	platform_device_register(&bcm63xx_gpio_leds);
--- a/arch/mips/include/asm/mach-bcm63xx/board_bcm963xx.h
+++ b/arch/mips/include/asm/mach-bcm63xx/board_bcm963xx.h
@@ -54,7 +54,7 @@ struct board_info {
 	struct bcm63xx_dsp_platform_data dsp;
 
 	/* GPIO LEDs */
-	struct gpio_led leds[5];
+	struct gpio_led leds[8];
 
 	/* Reset button */
 	struct gpio_button reset_buttons[1];
