--- a/drivers/net/wireless/ath/ath9k/ath9k.h
+++ b/drivers/net/wireless/ath/ath9k/ath9k.h
@@ -591,6 +591,7 @@ struct ath_softc {
 	struct ieee80211_hw *hw;
 	struct device *dev;
 
+	u32 chan_bw;
 	int chan_idx;
 	int chan_is_ht;
 	struct survey_info *cur_survey;
@@ -654,6 +655,7 @@ struct ath_softc {
 	u8 ant_tx, ant_rx;
 };
 
+int ath9k_config(struct ieee80211_hw *hw, u32 changed);
 void ath9k_tasklet(unsigned long data);
 int ath_cabq_update(struct ath_softc *);
 
--- a/drivers/net/wireless/ath/ath9k/debug.c
+++ b/drivers/net/wireless/ath/ath9k/debug.c
@@ -1663,6 +1663,50 @@ static const struct file_operations fops
 	.owner = THIS_MODULE
 };
 
+
+static ssize_t read_file_chan_bw(struct file *file, char __user *user_buf,
+			     size_t count, loff_t *ppos)
+{
+	struct ath_softc *sc = file->private_data;
+	char buf[32];
+	unsigned int len;
+
+	len = sprintf(buf, "0x%08x\n", sc->chan_bw);
+	return simple_read_from_buffer(user_buf, count, ppos, buf, len);
+}
+
+static ssize_t write_file_chan_bw(struct file *file, const char __user *user_buf,
+			     size_t count, loff_t *ppos)
+{
+	struct ath_softc *sc = file->private_data;
+	unsigned long chan_bw;
+	char buf[32];
+	ssize_t len;
+
+	len = min(count, sizeof(buf) - 1);
+	if (copy_from_user(buf, user_buf, len))
+		return -EFAULT;
+
+	buf[len] = '\0';
+	if (strict_strtoul(buf, 0, &chan_bw))
+		return -EINVAL;
+
+	sc->chan_bw = chan_bw;
+	if (!(sc->sc_flags & SC_OP_INVALID))
+		ath9k_config(sc->hw, IEEE80211_CONF_CHANGE_CHANNEL);
+
+	return count;
+}
+
+static const struct file_operations fops_chanbw = {
+	.read = read_file_chan_bw,
+	.write = write_file_chan_bw,
+	.open = ath9k_debugfs_open,
+	.owner = THIS_MODULE,
+	.llseek = default_llseek,
+};
+
+
 int ath9k_init_debug(struct ath_hw *ah)
 {
 	struct ath_common *common = ath9k_hw_common(ah);
@@ -1724,6 +1768,9 @@ int ath9k_init_debug(struct ath_hw *ah)
 	debugfs_create_file("eeprom", S_IRUSR, sc->debug.debugfs_phy, sc,
 			    &fops_eeprom);
 
+	debugfs_create_file("chanbw", S_IRUSR | S_IWUSR, sc->debug.debugfs_phy,
+			    sc, &fops_chanbw);
+
 	sc->debug.regidx = 0;
 	memset(&sc->debug.bb_mac_samp, 0, sizeof(sc->debug.bb_mac_samp));
 	sc->debug.sampidx = 0;
--- a/drivers/net/wireless/ath/ath9k/main.c
+++ b/drivers/net/wireless/ath/ath9k/main.c
@@ -1554,7 +1554,7 @@ static void ath9k_disable_ps(struct ath_
 
 }
 
-static int ath9k_config(struct ieee80211_hw *hw, u32 changed)
+int ath9k_config(struct ieee80211_hw *hw, u32 changed)
 {
 	struct ath_softc *sc = hw->priv;
 	struct ath_hw *ah = sc->sc_ah;
@@ -1606,9 +1606,10 @@ static int ath9k_config(struct ieee80211
 
 	if (changed & IEEE80211_CONF_CHANGE_CHANNEL) {
 		struct ieee80211_channel *curchan = hw->conf.channel;
-		struct ath9k_channel old_chan;
+		struct ath9k_channel old_chan, *hchan;
 		int pos = curchan->hw_value;
 		int old_pos = -1;
+		u32 oldflags;
 		unsigned long flags;
 
 		if (ah->curchan)
@@ -1661,7 +1662,23 @@ static int ath9k_config(struct ieee80211
 			memset(&sc->survey[pos], 0, sizeof(struct survey_info));
 		}
 
-		if (ath_set_channel(sc, hw, &sc->sc_ah->channels[pos]) < 0) {
+		hchan = &sc->sc_ah->channels[pos];
+		oldflags = hchan->channelFlags;
+		switch (sc->chan_bw) {
+		case 5:
+			hchan->channelFlags &= ~CHANNEL_HALF;
+			hchan->channelFlags |= CHANNEL_QUARTER;
+			break;
+		case 10:
+			hchan->channelFlags &= ~CHANNEL_QUARTER;
+			hchan->channelFlags |= CHANNEL_HALF;
+			break;
+		default:
+			hchan->channelFlags &= ~(CHANNEL_HALF | CHANNEL_QUARTER);
+			break;
+		}
+
+		if (ath_set_channel(sc, hw, hchan) < 0) {
 			ath_err(common, "Unable to set channel\n");
 			mutex_unlock(&sc->mutex);
 			return -EINVAL;
--- a/drivers/net/wireless/ath/ath9k/hw.c
+++ b/drivers/net/wireless/ath/ath9k/hw.c
@@ -1549,6 +1549,10 @@ int ath9k_hw_reset(struct ath_hw *ah, st
 	    caldata->rtt_hist.num_readings)
 		allow_fbs = true;
 
+	if (!ah->curchan || ((ah->curchan->channelFlags ^ chan->channelFlags) &
+	    (CHANNEL_HALF | CHANNEL_QUARTER)))
+		bChannelChange = false;
+
 	if (bChannelChange &&
 	    (ah->chip_fullsleep != true) &&
 	    (ah->curchan != NULL) &&
