--- a/drivers/usb/host/Kconfig
+++ b/drivers/usb/host/Kconfig
@@ -98,6 +98,13 @@ config USB_EHCI_BIG_ENDIAN_DESC
 	depends on USB_EHCI_HCD && (440EPX || ARCH_IXP4XX)
 	default y
 
+config USB_EHCI_AR71XX
+	bool "USB EHCI support for AR71xx"
+	depends on USB_EHCI_HCD && ATHEROS_AR71XX
+	default y
+	help
+	  Support for Atheros AR71xx built-in EHCI controller
+
 config USB_EHCI_FSL
 	bool "Support for Freescale on-chip EHCI USB controller"
 	depends on USB_EHCI_HCD && FSL_SOC
@@ -189,6 +196,13 @@ config USB_OHCI_HCD
 	  To compile this driver as a module, choose M here: the
 	  module will be called ohci-hcd.
 
+config USB_OHCI_AR71XX
+	bool "USB OHCI support for Atheros AR71xx"
+	depends on USB_OHCI_HCD && ATHEROS_AR71XX
+	default y
+	help
+	  Support for Atheros AR71xx built-in OHCI controller
+
 config USB_OHCI_HCD_PPC_SOC
 	bool "OHCI support for on-chip PPC USB controller"
 	depends on USB_OHCI_HCD && (STB03xxx || PPC_MPC52xx)
--- a/drivers/usb/host/ehci-hcd.c
+++ b/drivers/usb/host/ehci-hcd.c
@@ -1142,6 +1142,11 @@ MODULE_LICENSE ("GPL");
 #define	PLATFORM_DRIVER		ehci_atmel_driver
 #endif
 
+#ifdef CONFIG_USB_EHCI_AR71XX
+#include "ehci-ar71xx.c"
+#define PLATFORM_DRIVER		ehci_ar71xx_driver
+#endif
+
 #if !defined(PCI_DRIVER) && !defined(PLATFORM_DRIVER) && \
     !defined(PS3_SYSTEM_BUS_DRIVER) && !defined(OF_PLATFORM_DRIVER)
 #error "missing bus glue for ehci-hcd"
--- a/drivers/usb/host/ohci-hcd.c
+++ b/drivers/usb/host/ohci-hcd.c
@@ -1085,6 +1085,11 @@ MODULE_LICENSE ("GPL");
 #define TMIO_OHCI_DRIVER	ohci_hcd_tmio_driver
 #endif
 
+#ifdef CONFIG_USB_OHCI_AR71XX
+#include "ohci-ar71xx.c"
+#define PLATFORM_DRIVER		ohci_hcd_ar71xx_driver
+#endif
+
 #if	!defined(PCI_DRIVER) &&		\
 	!defined(PLATFORM_DRIVER) &&	\
 	!defined(OF_PLATFORM_DRIVER) &&	\
