--- a/arch/mips/Kconfig
+++ b/arch/mips/Kconfig
@@ -39,6 +39,23 @@ choice
 	prompt "System type"
 	default SGI_IP22
 
+config ADM5120
+	bool "Infineon/ADMtek ADM5120 SoC based machines"
+	select BOOT_RAW
+	select NO_EXCEPT_FILL
+	select CEVT_R4K
+	select CSRC_R4K
+	select SYS_HAS_CPU_MIPS32_R1
+	select SYS_HAS_EARLY_PRINTK
+	select DMA_NONCOHERENT
+	select IRQ_CPU
+	select SYS_SUPPORTS_LITTLE_ENDIAN
+	select SYS_SUPPORTS_BIG_ENDIAN
+	select SYS_SUPPORTS_32BIT_KERNEL
+	select ARCH_REQUIRE_GPIOLIB
+	select SWAP_IO_SPACE if CPU_BIG_ENDIAN
+	select MIPS_MACHINE
+
 config MIPS_ALCHEMY
 	bool "Alchemy processor based machines"
 	select 64BIT_PHYS_ADDR
@@ -813,6 +830,7 @@ config NLM_XLP_BOARD
 
 endchoice
 
+source "arch/mips/adm5120/Kconfig"
 source "arch/mips/alchemy/Kconfig"
 source "arch/mips/ath79/Kconfig"
 source "arch/mips/bcm47xx/Kconfig"
--- a/arch/mips/Kbuild.platforms
+++ b/arch/mips/Kbuild.platforms
@@ -1,5 +1,6 @@
 # All platforms listed in alphabetic order
 
+platforms += adm5120
 platforms += alchemy
 platforms += ar7
 platforms += ath79
