From 98bfbb0b3f126d93076377fcd9553a493e45e304 Mon Sep 17 00:00:00 2001
From: Gabor Juhos <juhosg@openwrt.org>
Date: Wed, 14 Mar 2012 10:45:26 +0100
Subject: [PATCH 31/47] MIPS: ath79: add AR934X specific glue to ath79_device_reset_{clear,set}

Signed-off-by: Gabor Juhos <juhosg@openwrt.org>
Acked-by: Luis R. Rodriguez <mcgrof@qca.qualcomm.com>
Cc: linux-mips@linux-mips.org
Cc: mcgrof@infradead.org
Patchwork: https://patchwork.linux-mips.org/patch/3511/
Signed-off-by: Ralf Baechle <ralf@linux-mips.org>
---
 arch/mips/ath79/common.c                       |    9 ++++++++-
 arch/mips/include/asm/mach-ath79/ar71xx_regs.h |    1 +
 2 files changed, 9 insertions(+), 1 deletions(-)

--- a/arch/mips/ath79/common.c
+++ b/arch/mips/ath79/common.c
@@ -1,9 +1,12 @@
 /*
  *  Atheros AR71XX/AR724X/AR913X common routines
  *
- *  Copyright (C) 2008-2010 Gabor Juhos <juhosg@openwrt.org>
+ *  Copyright (C) 2010-2011 Jaiganesh Narayanan <jnarayanan@atheros.com>
+ *  Copyright (C) 2008-2011 Gabor Juhos <juhosg@openwrt.org>
  *  Copyright (C) 2008 Imre Kaloz <kaloz@openwrt.org>
  *
+ *  Parts of this file are based on Atheros' 2.6.15/2.6.31 BSP
+ *
  *  This program is free software; you can redistribute it and/or modify it
  *  under the terms of the GNU General Public License version 2 as published
  *  by the Free Software Foundation.
@@ -67,6 +70,8 @@ void ath79_device_reset_set(u32 mask)
 		reg = AR913X_RESET_REG_RESET_MODULE;
 	else if (soc_is_ar933x())
 		reg = AR933X_RESET_REG_RESET_MODULE;
+	else if (soc_is_ar934x())
+		reg = AR934X_RESET_REG_RESET_MODULE;
 	else
 		BUG();
 
@@ -91,6 +96,8 @@ void ath79_device_reset_clear(u32 mask)
 		reg = AR913X_RESET_REG_RESET_MODULE;
 	else if (soc_is_ar933x())
 		reg = AR933X_RESET_REG_RESET_MODULE;
+	else if (soc_is_ar934x())
+		reg = AR934X_RESET_REG_RESET_MODULE;
 	else
 		BUG();
 
--- a/arch/mips/include/asm/mach-ath79/ar71xx_regs.h
+++ b/arch/mips/include/asm/mach-ath79/ar71xx_regs.h
@@ -227,6 +227,7 @@
 #define AR933X_RESET_REG_RESET_MODULE		0x1c
 #define AR933X_RESET_REG_BOOTSTRAP		0xac
 
+#define AR934X_RESET_REG_RESET_MODULE		0x1c
 #define AR934X_RESET_REG_BOOTSTRAP		0xb0
 #define AR934X_RESET_REG_PCIE_WMAC_INT_STATUS	0xac
 
