From d0ae5f33c0221339a50bd1005c569934417003a5 Mon Sep 17 00:00:00 2001
From: Daniel Golle <dgolle@allnet.de>
Date: Thu, 4 Oct 2012 00:34:01 +0200
Subject: [PATCH] rt2x00/rt3352: Fix lnagain assignment to use register 66.
To: users@rt2x00.serialmonkey.com
Cc: gwingerde@gmail.com

---
 drivers/net/wireless/rt2x00/rt2800lib.c | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/drivers/net/wireless/rt2x00/rt2800lib.c
+++ b/drivers/net/wireless/rt2x00/rt2800lib.c
@@ -2273,9 +2273,9 @@ static void rt2800_config_channel(struct
 	 */
 	if (rt2x00_rt(rt2x00dev, RT3352)) {
 		rt2800_bbp_write(rt2x00dev, 27, 0x0);
-		rt2800_bbp_write(rt2x00dev, 62, 0x26 + rt2x00dev->lna_gain);
+		rt2800_bbp_write(rt2x00dev, 66, 0x26 + rt2x00dev->lna_gain);
 		rt2800_bbp_write(rt2x00dev, 27, 0x20);
-		rt2800_bbp_write(rt2x00dev, 62, 0x26 + rt2x00dev->lna_gain);
+		rt2800_bbp_write(rt2x00dev, 66, 0x26 + rt2x00dev->lna_gain);
 	} else {
 		rt2800_bbp_write(rt2x00dev, 62, 0x37 - rt2x00dev->lna_gain);
 		rt2800_bbp_write(rt2x00dev, 63, 0x37 - rt2x00dev->lna_gain);
