#!/bin/sh /etc/rc.common


. /lib/functions/network.sh

START=50

SERVICE_DAEMONIZE=1
SERVICE_WRITE_PID=1

start_daemon() {
	local cfg="$1"

	local atmdev
	config_get atmdev "$cfg" atmdev 0

	local unit
	config_get unit "$cfg" unit 0

	local vpi
	config_get vpi "$cfg" vpi 8

	local vci
	config_get vci "$cfg" vci 35

	local encaps
	config_get encaps "$cfg" encaps

	case "$encaps" in
		1|vc) encaps=1;;
		*) encaps=0;;
	esac

	local payload
	config_get payload "$cfg" payload

	case "$payload" in
		0|routed) payload=0;;
		*) payload=1;;
	esac

	local qos
	config_get qos "$cfg" qos

	local sendsize
	config_get sendsize "$cfg" sendsize

	local circuit="$atmdev.$vpi.$vci"

	network_defer_device "nas$unit"

	SERVICE_PID_FILE="/var/run/br2684ctl-$circuit.pid" \
	service_start /usr/sbin/br2684ctl \
		-c "$unit" -e "$encaps" -p "$payload" \
		-a "$circuit" ${qos:+-q "$qos"} ${sendsize:+-s "$sendsize"}
	sleep 1

	network_ready_device "nas$unit"
}

stop_daemon() {
	local cfg="$1"

	local atmdev
	config_get atmdev "$cfg" atmdev 0

	local unit
	config_get unit "$cfg" unit 0

	local vpi
	config_get vpi "$cfg" vpi 8

	local vci
	config_get vci "$cfg" vci 35

	local circuit="$atmdev.$vpi.$vci"
	
	SERVICE_PID_FILE="/var/run/br2684ctl-$circuit.pid" \
	service_stop /usr/sbin/br2684ctl
}

start() {
	config_load network
	config_foreach start_daemon atm-bridge
}

stop() {
	config_load network
	config_foreach stop_daemon atm-bridge
}
