From c3a8b5fa196cedc4b940c1e5ec482dd875aa3180 Mon Sep 17 00:00:00 2001
From: Gabor Juhos <juhosg@openwrt.org>
Date: Mon, 11 Jun 2012 13:38:06 +0200
Subject: [PATCH 06/34] MIPS: ath79: move global PCI defines into a common header

The constants will be used by a subsequent patch.

Signed-off-by: Gabor Juhos <juhosg@openwrt.org>
---
 arch/mips/include/asm/mach-ath79/ar71xx_regs.h |   24 ++++++++++++++++++++++++
 arch/mips/pci/pci-ar71xx.c                     |   16 ----------------
 arch/mips/pci/pci-ar724x.c                     |    8 --------
 3 files changed, 24 insertions(+), 24 deletions(-)

--- a/arch/mips/include/asm/mach-ath79/ar71xx_regs.h
+++ b/arch/mips/include/asm/mach-ath79/ar71xx_regs.h
@@ -41,11 +41,35 @@
 #define AR71XX_RESET_BASE	(AR71XX_APB_BASE + 0x00060000)
 #define AR71XX_RESET_SIZE	0x100
 
+#define AR71XX_PCI_MEM_BASE	0x10000000
+#define AR71XX_PCI_MEM_SIZE	0x07000000
+
+#define AR71XX_PCI_WIN0_OFFS	0x10000000
+#define AR71XX_PCI_WIN1_OFFS	0x11000000
+#define AR71XX_PCI_WIN2_OFFS	0x12000000
+#define AR71XX_PCI_WIN3_OFFS	0x13000000
+#define AR71XX_PCI_WIN4_OFFS	0x14000000
+#define AR71XX_PCI_WIN5_OFFS	0x15000000
+#define AR71XX_PCI_WIN6_OFFS	0x16000000
+#define AR71XX_PCI_WIN7_OFFS	0x07000000
+
+#define AR71XX_PCI_CFG_BASE	\
+	(AR71XX_PCI_MEM_BASE + AR71XX_PCI_WIN7_OFFS + 0x10000)
+#define AR71XX_PCI_CFG_SIZE	0x100
+
 #define AR7240_USB_CTRL_BASE	(AR71XX_APB_BASE + 0x00030000)
 #define AR7240_USB_CTRL_SIZE	0x100
 #define AR7240_OHCI_BASE	0x1b000000
 #define AR7240_OHCI_SIZE	0x1000
 
+#define AR724X_PCI_MEM_BASE	0x10000000
+#define AR724X_PCI_MEM_SIZE	0x04000000
+
+#define AR724X_PCI_CFG_BASE	0x14000000
+#define AR724X_PCI_CFG_SIZE	0x1000
+#define AR724X_PCI_CTRL_BASE	(AR71XX_APB_BASE + 0x000f0000)
+#define AR724X_PCI_CTRL_SIZE	0x100
+
 #define AR724X_EHCI_BASE	0x1b000000
 #define AR724X_EHCI_SIZE	0x1000
 
--- a/arch/mips/pci/pci-ar71xx.c
+++ b/arch/mips/pci/pci-ar71xx.c
@@ -25,22 +25,6 @@
 #include <asm/mach-ath79/ath79.h>
 #include <asm/mach-ath79/pci.h>
 
-#define AR71XX_PCI_MEM_BASE	0x10000000
-#define AR71XX_PCI_MEM_SIZE	0x07000000
-
-#define AR71XX_PCI_WIN0_OFFS		0x10000000
-#define AR71XX_PCI_WIN1_OFFS		0x11000000
-#define AR71XX_PCI_WIN2_OFFS		0x12000000
-#define AR71XX_PCI_WIN3_OFFS		0x13000000
-#define AR71XX_PCI_WIN4_OFFS		0x14000000
-#define AR71XX_PCI_WIN5_OFFS		0x15000000
-#define AR71XX_PCI_WIN6_OFFS		0x16000000
-#define AR71XX_PCI_WIN7_OFFS		0x07000000
-
-#define AR71XX_PCI_CFG_BASE		\
-	(AR71XX_PCI_MEM_BASE + AR71XX_PCI_WIN7_OFFS + 0x10000)
-#define AR71XX_PCI_CFG_SIZE		0x100
-
 #define AR71XX_PCI_REG_CRP_AD_CBE	0x00
 #define AR71XX_PCI_REG_CRP_WRDATA	0x04
 #define AR71XX_PCI_REG_CRP_RDDATA	0x08
--- a/arch/mips/pci/pci-ar724x.c
+++ b/arch/mips/pci/pci-ar724x.c
@@ -17,14 +17,6 @@
 #include <asm/mach-ath79/ar71xx_regs.h>
 #include <asm/mach-ath79/pci.h>
 
-#define AR724X_PCI_CFG_BASE	0x14000000
-#define AR724X_PCI_CFG_SIZE	0x1000
-#define AR724X_PCI_CTRL_BASE	(AR71XX_APB_BASE + 0x000f0000)
-#define AR724X_PCI_CTRL_SIZE	0x100
-
-#define AR724X_PCI_MEM_BASE	0x10000000
-#define AR724X_PCI_MEM_SIZE	0x04000000
-
 #define AR724X_PCI_REG_RESET		0x18
 #define AR724X_PCI_REG_INT_STATUS	0x4c
 #define AR724X_PCI_REG_INT_MASK		0x50
