From 2cae40a6a76e9e440f146ce0402aed40a7c127ca Mon Sep 17 00:00:00 2001
From: San Mehat <san@google.com>
Date: Mon, 10 Nov 2008 16:29:50 -0800
Subject: [PATCH 093/134] mmc: Add status IRQ and status callback function to mmc platform data

Signed-off-by: San Mehat <san@google.com>
---
 arch/arm/include/asm/mach/mmc.h |    2 ++
 1 files changed, 2 insertions(+), 0 deletions(-)

--- a/arch/arm/include/asm/mach/mmc.h
+++ b/arch/arm/include/asm/mach/mmc.h
@@ -10,6 +10,8 @@ struct mmc_platform_data {
 	unsigned int ocr_mask;			/* available voltages */
 	u32 (*translate_vdd)(struct device *, unsigned int);
 	unsigned int (*status)(struct device *);
+	unsigned int status_irq;
+	int (*register_status_notify)(void (*callback)(int card_present, void *dev_id), void *dev_id);
 };
 
 #endif
