--- /dev/null
+++ b/drivers/usb/host/ehci-cns21xx.c
@@ -0,0 +1,186 @@
+/*
+ *  Copyright (c) 2008 Cavium Networks
+ *  Copyright (c) 2010-2012 Gabor Juhos <juhosg@openwrt.org>
+ *
+ *  This file is free software; you can redistribute it and/or modify
+ *  it under the terms of the GNU General Public License, Version 2, as
+ *  published by the Free Software Foundation.
+ */
+
+#include <linux/platform_device.h>
+#include <linux/irq.h>
+
+#include <mach/cns21xx.h>
+
+#define DRIVER_NAME	"cns21xx-ehci"
+
+static int cns21xx_ehci_reset(struct usb_hcd *hcd)
+{
+	struct ehci_hcd *ehci = hcd_to_ehci(hcd);
+	int ret;
+
+	ret = ehci_halt(ehci);
+	if (ret)
+		return ret;
+
+	ret = ehci_init(hcd);
+	if (ret)
+		return ret;
+
+	ehci_reset(ehci);
+	ehci_port_power(ehci, 0);
+
+	return 0;
+}
+
+static const struct hc_driver ehci_cns21xx_hc_driver = {
+	.description		= hcd_name,
+        .product_desc		= DRIVER_NAME,
+        .hcd_priv_size		= sizeof(struct ehci_hcd),
+
+	/*
+	 * generic hardware linkage
+	 */
+	.irq			= ehci_irq,
+	.flags			= HCD_MEMORY | HCD_USB2,
+
+	/*
+	 * basic lifecycle operations
+	 */
+	.reset			= cns21xx_ehci_reset,
+	.start			= ehci_run,
+	.stop			= ehci_stop,
+	.shutdown		= ehci_shutdown,
+
+	/*
+	 * managing i/o requests and associated device resources
+	 */
+	.urb_enqueue		= ehci_urb_enqueue,
+	.urb_dequeue		= ehci_urb_dequeue,
+	.endpoint_disable	= ehci_endpoint_disable,
+	.endpoint_reset		= ehci_endpoint_reset,
+
+	/*
+	 * scheduling support
+	 */
+	.get_frame_number	= ehci_get_frame,
+
+	/*
+	 * root hub support
+	 */
+	.hub_status_data	= ehci_hub_status_data,
+	.hub_control		= ehci_hub_control,
+	.relinquish_port	= ehci_relinquish_port,
+	.port_handed_over	= ehci_port_handed_over,
+
+	.clear_tt_buffer_complete = ehci_clear_tt_buffer_complete,
+};
+
+static void cns21xx_ehci_init_hc(void)
+{
+	__raw_writel(0x106, CNS21XX_EHCI_CONFIG_BASE_VIRT + 0x04);
+	__raw_writel((3 << 5) | 0x2000, CNS21XX_EHCI_CONFIG_BASE_VIRT + 0x40);
+	msleep(100);
+}
+
+static int ehci_cns21xx_probe(struct platform_device *pdev)
+{
+	struct usb_hcd *hcd;
+	struct ehci_hcd *ehci;
+	struct resource *res;
+	int irq;
+	int ret;
+
+	if (usb_disabled())
+		return -ENODEV;
+
+	res = platform_get_resource(pdev, IORESOURCE_IRQ, 0);
+	if (!res) {
+		dev_dbg(&pdev->dev, "no IRQ specified for %s\n",
+			dev_name(&pdev->dev));
+		return -ENODEV;
+	}
+	irq = res->start;
+
+	hcd = usb_create_hcd(&ehci_cns21xx_hc_driver, &pdev->dev,
+			     dev_name(&pdev->dev));
+	if (!hcd)
+		return -ENOMEM;
+
+	res = platform_get_resource(pdev, IORESOURCE_MEM, 0);
+	if (!res) {
+		dev_dbg(&pdev->dev, "no base address specified for %s\n",
+			dev_name(&pdev->dev));
+		ret = -ENODEV;
+		goto err_put_hcd;
+	}
+	hcd->rsrc_start	= res->start;
+	hcd->rsrc_len	= res->end - res->start + 1;
+
+	if (!request_mem_region(hcd->rsrc_start, hcd->rsrc_len, hcd_name)) {
+		dev_dbg(&pdev->dev, "controller already in use\n");
+		ret = -EBUSY;
+		goto err_put_hcd;
+	}
+
+	hcd->regs = ioremap(hcd->rsrc_start, hcd->rsrc_len);
+	if (!hcd->regs) {
+		dev_dbg(&pdev->dev, "error mapping memory\n");
+		ret = -EFAULT;
+		goto err_release_region;
+	}
+
+	cns21xx_ehci_init_hc();
+
+	ehci = hcd_to_ehci(hcd);
+
+	ehci->caps = hcd->regs;
+	ehci->regs = hcd->regs +
+		     HC_LENGTH(ehci, ehci_readl(ehci, &ehci->caps->hc_capbase));
+	dbg_hcs_params(ehci, "reset");
+	dbg_hcc_params(ehci, "reset");
+
+	/* cache this readonly data; minimize chip reads */
+	ehci->hcs_params = readl(&ehci->caps->hcs_params);
+	ehci->sbrn = 0x20;
+
+	ret = usb_add_hcd(hcd, CNS21XX_IRQ_EHCI, IRQF_DISABLED);
+	if (ret)
+		goto err_unmap;
+
+	platform_set_drvdata(pdev, hcd);
+	return 0;
+
+err_unmap:
+	iounmap(hcd->regs);
+err_release_region:
+	release_mem_region(hcd->rsrc_start, hcd->rsrc_len);
+err_put_hcd:
+	usb_put_hcd(hcd);
+	return ret;
+}
+
+static int ehci_cns21xx_remove(struct platform_device *pdev)
+{
+	struct usb_hcd *hcd = platform_get_drvdata(pdev);
+
+	usb_remove_hcd(hcd);
+	iounmap(hcd->regs);
+	release_mem_region(hcd->rsrc_start, hcd->rsrc_len);
+	usb_put_hcd(hcd);
+	platform_set_drvdata(pdev, NULL);
+
+	return 0;
+}
+
+static struct platform_driver ehci_cns21xx_driver = {
+	.probe		= ehci_cns21xx_probe,
+	.remove		= ehci_cns21xx_remove,
+	.shutdown       = usb_hcd_platform_shutdown,
+	.driver		= {
+		.owner	= THIS_MODULE,
+		.name	= DRIVER_NAME,
+	},
+};
+
+MODULE_ALIAS("platform:" DRIVER_NAME);
--- a/drivers/usb/host/ehci-hcd.c
+++ b/drivers/usb/host/ehci-hcd.c
@@ -1376,6 +1376,11 @@ MODULE_LICENSE ("GPL");
 #define        PLATFORM_DRIVER         ehci_mv_driver
 #endif
 
+#ifdef CONFIG_ARCH_CNS21XX
+#include "ehci-cns21xx.c"
+#define PLATFORM_DRIVER		ehci_cns21xx_driver
+#endif
+
 #if !defined(PCI_DRIVER) && !defined(PLATFORM_DRIVER) && \
     !defined(PS3_SYSTEM_BUS_DRIVER) && !defined(OF_PLATFORM_DRIVER) && \
     !defined(XILINX_OF_PLATFORM_DRIVER)
--- a/arch/arm/Kconfig
+++ b/arch/arm/Kconfig
@@ -369,6 +369,7 @@ config ARCH_CNS21XX
 	select ARCH_REQUIRE_GPIOLIB
 	select ARM_L1_CACHE_SHIFT_4
 	select USB_ARCH_HAS_OHCI
+	select USB_ARCH_HAS_EHCI
 	help
 	  Support for Cavium Networks CNS21xx family.
 
