--- a/arch/arm/mach-ixp4xx/gtwx5715-setup.c
+++ b/arch/arm/mach-ixp4xx/gtwx5715-setup.c
@@ -178,10 +178,37 @@ static struct platform_device gtwx5715_s
 	},
 };
 
+static struct eth_plat_info gtwx5715_npeb_data = {
+	.phy		= IXP4XX_ETH_PHY_MAX_ADDR,
+	.phy_mask	= 0x1e, /* ports 1-4 of the KS8995 switch */
+	.rxq		= 3,
+	.txreadyq	= 20,
+};
+
+static struct eth_plat_info gtwx5715_npec_data = {
+	.phy		= 5,	/* port 5 of the KS8995 switch */
+	.rxq		= 4,
+	.txreadyq	= 21,
+};
+
+static struct platform_device gtwx5715_npeb_device = {
+	.name			= "ixp4xx_eth",
+	.id			= IXP4XX_ETH_NPEB,
+	.dev.platform_data	= &gtwx5715_npeb_data,
+};
+
+static struct platform_device gtwx5715_npec_device = {
+	.name			= "ixp4xx_eth",
+	.id			= IXP4XX_ETH_NPEC,
+	.dev.platform_data	= &gtwx5715_npec_data,
+};
+
 static struct platform_device *gtwx5715_devices[] __initdata = {
 	&gtwx5715_uart_device,
 	&gtwx5715_flash,
 	&gtwx5715_spi_bus,
+	&gtwx5715_npeb_device,
+	&gtwx5715_npec_device,
 };
 
 static void __init gtwx5715_init(void)
