From 8d2a7d1fb561c9cb098c2b13ded34fe0f49dcca5 Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Fri, 3 Aug 2012 10:27:25 +0200
Subject: [PATCH 20/25] owrt atm

---
 arch/mips/lantiq/irq.c |    2 ++
 arch/mips/mm/cache.c   |    2 ++
 net/atm/common.c       |    6 ++++++
 net/atm/proc.c         |    2 +-
 4 files changed, 11 insertions(+), 1 deletions(-)

diff --git a/arch/mips/lantiq/irq.c b/arch/mips/lantiq/irq.c
index 63dbb83..1e89104 100644
--- a/arch/mips/lantiq/irq.c
+++ b/arch/mips/lantiq/irq.c
@@ -10,6 +10,7 @@
 #include <linux/interrupt.h>
 #include <linux/ioport.h>
 #include <linux/sched.h>
+#include <linux/module.h>
 
 #include <asm/bootinfo.h>
 #include <asm/irq_cpu.h>
@@ -171,6 +172,7 @@ void ltq_disable_irq(struct irq_data *d)
 	ltq_icu_w32(ltq_icu_r32(LTQ_ICU_IM0_IER, im_nr) & ~(1 << irq_nr),
 		LTQ_ICU_IM0_IER, im_nr);
 }
+EXPORT_SYMBOL(ltq_mask_and_ack_irq);
 
 void ltq_mask_and_ack_irq(struct irq_data *d)
 {
diff --git a/arch/mips/mm/cache.c b/arch/mips/mm/cache.c
index ef83ef1..c156456 100644
--- a/arch/mips/mm/cache.c
+++ b/arch/mips/mm/cache.c
@@ -58,6 +58,8 @@ void (*_dma_cache_wback)(unsigned long start, unsigned long size);
 void (*_dma_cache_inv)(unsigned long start, unsigned long size);
 
 EXPORT_SYMBOL(_dma_cache_wback_inv);
+EXPORT_SYMBOL(_dma_cache_wback);
+EXPORT_SYMBOL(_dma_cache_inv);
 
 #endif /* CONFIG_DMA_NONCOHERENT */
 
diff --git a/net/atm/common.c b/net/atm/common.c
index b4b44db..c30b397 100644
--- a/net/atm/common.c
+++ b/net/atm/common.c
@@ -62,11 +62,17 @@ static void vcc_remove_socket(struct sock *sk)
 	write_unlock_irq(&vcc_sklist_lock);
 }
 
+struct sk_buff* (*ifx_atm_alloc_tx)(struct atm_vcc *, unsigned int) = NULL;
+EXPORT_SYMBOL(ifx_atm_alloc_tx);
+
 static struct sk_buff *alloc_tx(struct atm_vcc *vcc, unsigned int size)
 {
 	struct sk_buff *skb;
 	struct sock *sk = sk_atm(vcc);
 
+	if (ifx_atm_alloc_tx != NULL)
+		return ifx_atm_alloc_tx(vcc, size);
+
 	if (sk_wmem_alloc_get(sk) && !atm_may_send(vcc, size)) {
 		pr_debug("Sorry: wmem_alloc = %d, size = %d, sndbuf = %d\n",
 			 sk_wmem_alloc_get(sk), size, sk->sk_sndbuf);
diff --git a/net/atm/proc.c b/net/atm/proc.c
index 0d020de..9fdb539 100644
--- a/net/atm/proc.c
+++ b/net/atm/proc.c
@@ -154,7 +154,7 @@ static void *vcc_seq_next(struct seq_file *seq, void *v, loff_t *pos)
 static void pvc_info(struct seq_file *seq, struct atm_vcc *vcc)
 {
 	static const char *const class_name[] = {
-		"off", "UBR", "CBR", "VBR", "ABR"};
+		"off","UBR","CBR","NTR-VBR","ABR","ANY","RT-VBR","UBR+","GFR"};
 	static const char *const aal_name[] = {
 		"---",	"1",	"2",	"3/4",	/*  0- 3 */
 		"???",	"5",	"???",	"???",	/*  4- 7 */
-- 
1.7.9.1

