From ffc4445958a3ed4064f2e1bf73fa478a61c5cf7b Mon Sep 17 00:00:00 2001
From: Antonio Quartulli <ordex@autistici.org>
Date: Sun, 3 Jun 2012 18:42:25 +0200
Subject: [PATCHv2 602/602] driver_nl80211: use new parameters during ibss join

Signed-hostap: Antonio Quartulli <ordex@autistici.org>
---
 src/drivers/driver_nl80211.c |   33 ++++++++++++++++++++++++++++++++-
 1 file changed, 32 insertions(+), 1 deletion(-)

--- a/src/drivers/driver_nl80211.c
+++ b/src/drivers/driver_nl80211.c
@@ -6587,7 +6587,7 @@ static int wpa_driver_nl80211_ibss(struc
 				   struct wpa_driver_associate_params *params)
 {
 	struct nl_msg *msg;
-	int ret = -1;
+	int ret = -1, i;
 	int count = 0;
 
 	wpa_printf(MSG_DEBUG, "nl80211: Join IBSS (ifindex=%d)", drv->ifindex);
@@ -6620,6 +6620,37 @@ retry:
 	wpa_printf(MSG_DEBUG, "  * freq=%d", params->freq);
 	NLA_PUT_U32(msg, NL80211_ATTR_WIPHY_FREQ, params->freq);
 
+	if (params->fixed_freq) {
+		wpa_printf(MSG_DEBUG, "  * fixed_freq");
+		NLA_PUT_FLAG(msg, NL80211_ATTR_FREQ_FIXED);
+	}
+
+	if (params->beacon_interval > 0) {
+		wpa_printf(MSG_DEBUG, "  * beacon_interval=%d",
+			   params->beacon_interval);
+		NLA_PUT_U32(msg, NL80211_ATTR_BEACON_INTERVAL,
+			    params->beacon_interval);
+	}
+
+	if (params->rates[0] > 0) {
+		wpa_printf(MSG_DEBUG, "  * basic_rates:");
+		i = 0;
+		while (i < NL80211_MAX_SUPP_RATES &&
+		       params->rates[i] > 0) {
+			wpa_printf(MSG_DEBUG, "    %.1f",
+				   (double)params->rates[i] / 2);
+			i++;
+		}
+		NLA_PUT(msg, NL80211_ATTR_BSS_BASIC_RATES, i,
+			params->rates);
+	}
+
+	if (params->mcast_rate > 0) {
+		wpa_printf(MSG_DEBUG, "  * mcast_rates=%.1f",
+			   (double)params->mcast_rate / 10);
+		NLA_PUT_U32(msg, NL80211_ATTR_MCAST_RATE, params->mcast_rate);
+	}
+
 	ret = nl80211_set_conn_keys(params, msg);
 	if (ret)
 		goto nla_put_failure;
