--- a/arch/mips/bcm47xx/Kconfig
+++ b/arch/mips/bcm47xx/Kconfig
@@ -21,6 +21,7 @@ config BCM47XX_BCMA
 	select BCMA
 	select BCMA_HOST_SOC
 	select BCMA_DRIVER_MIPS
+	select BCMA_HOST_PCI if PCI
 	select BCMA_DRIVER_PCI_HOSTMODE if PCI
 	default y
 	help
