From 2d4ed1c7405d05da812b67830eaac15f43b862b7 Mon Sep 17 00:00:00 2001
From: Gabor Juhos <juhosg@openwrt.org>
Date: Wed, 14 Mar 2012 10:45:27 +0100
Subject: [PATCH 32/47] MIPS: ath79: register UART device for AR934X SoCs

Signed-off-by: Gabor Juhos <juhosg@openwrt.org>
Acked-by: Luis R. Rodriguez <mcgrof@qca.qualcomm.com>
Cc: linux-mips@linux-mips.org
Cc: mcgrof@infradead.org
Patchwork: https://patchwork.linux-mips.org/patch/3512/
Signed-off-by: Ralf Baechle <ralf@linux-mips.org>
---
 arch/mips/ath79/dev-common.c |    3 ++-
 1 files changed, 2 insertions(+), 1 deletions(-)

--- a/arch/mips/ath79/dev-common.c
+++ b/arch/mips/ath79/dev-common.c
@@ -89,7 +89,8 @@ void __init ath79_register_uart(void)
 
 	if (soc_is_ar71xx() ||
 	    soc_is_ar724x() ||
-	    soc_is_ar913x()) {
+	    soc_is_ar913x() ||
+	    soc_is_ar934x()) {
 		ath79_uart_data[0].uartclk = clk_get_rate(clk);
 		platform_device_register(&ath79_uart_device);
 	} else if (soc_is_ar933x()) {
